<!--startmeta
custom_edit_url: "https://github.com/netdata/netdata/edit/master/src/collectors/python.d.plugin/am2320/README.md"
meta_yaml: "https://github.com/netdata/netdata/edit/master/src/collectors/python.d.plugin/am2320/metadata.yaml"
sidebar_label: "AM2320"
learn_status: "Published"
learn_rel_path: "Collecting Metrics/Collectors/Hardware and Sensors"
keywords: ['temperature', 'am2320', 'sensor', 'humidity']
message: "DO NOT EDIT THIS FILE DIRECTLY, IT IS GENERATED BY THE COLLECTOR'S metadata.yaml FILE"
endmeta-->

# AM2320


<img src="https://netdata.cloud/img/microchip.svg" width="150"/>


Plugin: python.d.plugin
Module: am2320

<img src="https://img.shields.io/badge/maintained%20by-Netdata-%2300ab44" />

## Overview

This collector monitors AM2320 sensor metrics about temperature and humidity.

It retrieves temperature and humidity values by contacting an AM2320 sensor over i2c.

This collector is supported on all platforms.

This collector only supports collecting metrics from a single instance of this integration.


### Default Behavior

#### Auto-Detection

Assuming prerequisites are met, the collector will try to connect to the sensor via i2c

#### Limits

The default configuration for this integration does not impose any limits on data collection.

#### Performance Impact

The default configuration for this integration is not expected to impose a significant performance impact on the system.

## Setup


### Prerequisites

#### Sensor connection to a Raspberry Pi

Connect the am2320 to the Raspberry Pi I2C pins

Raspberry Pi 3B/4 Pins:

- Board 3.3V (pin 1) to sensor VIN (pin 1)
- Board SDA (pin 3) to sensor SDA (pin 2)
- Board GND (pin 6) to sensor GND (pin 3)
- Board SCL (pin 5) to sensor SCL (pin 4)

You may also need to add two I2C pullup resistors if your board does not already have them. The Raspberry Pi does have internal pullup resistors but it doesn't hurt to add them anyway. You can use 2.2K - 10K but we will just use 10K. The resistors go from VDD to SCL and SDA each.


#### Software requirements

Install the Adafruit Circuit Python AM2320 library:

`sudo pip3 install adafruit-circuitpython-am2320`



### Configuration

#### Options

There are 2 sections:

* Global variables
* One or more JOBS that can define multiple different instances to monitor.

The following options can be defined globally: priority, penalty, autodetection_retry, update_every, but can also be defined per JOB to override the global values.

Additionally, the following collapsed table contains all the options that can be configured inside a JOB definition.

Every configuration JOB starts with a `job_name` value which will appear in the dashboard, unless a `name` parameter is specified.


<details open><summary>Config options</summary>



| Option | Description | Default | Required |
|:-----|:------------|:--------|:---------:|
| update_every | Sets the default data collection frequency. | 5 | no |
| priority | Controls the order of charts at the netdata dashboard. | 60000 | no |
| autodetection_retry | Sets the job re-check interval in seconds. | 0 | no |
| penalty | Indicates whether to apply penalty to update_every in case of failures. | yes | no |
| name | Job name. This value will overwrite the `job_name` value. JOBS with the same name are mutually exclusive. Only one of them will be allowed running at any time. This allows autodetection to try several alternatives and pick the one that works. |  | no |


</details>



#### via File

The configuration file name for this integration is `python.d/am2320.conf`.

The file format is YAML. Generally, the structure is:

```yaml
update_every: 1
autodetection_retry: 0

job_name:
  job_option1: some_value
  job_option2: some_other_vlaue
```
You can edit the configuration file using the [`edit-config`](https://github.com/netdata/netdata/blob/master/docs/netdata-agent/configuration/README.md#edit-configuration-files) script from the
Netdata [config directory](https://github.com/netdata/netdata/blob/master/docs/netdata-agent/configuration/README.md#locate-your-config-directory).

```bash
cd /etc/netdata 2>/dev/null || cd /opt/netdata/etc/netdata
sudo ./edit-config python.d/am2320.conf
```

##### Examples

###### Local sensor

A basic JOB configuration

```yaml
local_sensor:
  name: 'Local AM2320'

```


## Alerts

There are no alerts configured by default for this integration.


## Metrics

Metrics grouped by *scope*.

The scope defines the instance that the metric belongs to. An instance is uniquely identified by a set of labels.



### Per AM2320 instance

These metrics refer to the entire monitored application.

This scope has no labels.

Metrics:

| Metric | Dimensions | Unit |
|:------|:----------|:----|
| am2320.temperature | temperature | celsius |
| am2320.humidity | humidity | percentage |



## Troubleshooting

### Debug Mode


To troubleshoot issues with the `am2320` collector, run the `python.d.plugin` with the debug option enabled. The output
should give you clues as to why the collector isn't working.

- Navigate to the `plugins.d` directory, usually at `/usr/libexec/netdata/plugins.d/`. If that's not the case on
  your system, open `netdata.conf` and look for the `plugins` setting under `[directories]`.

  ```bash
  cd /usr/libexec/netdata/plugins.d/
  ```

- Switch to the `netdata` user.

  ```bash
  sudo -u netdata -s
  ```

- Run the `python.d.plugin` to debug the collector:

  ```bash
  ./python.d.plugin am2320 debug trace
  ```

### Getting Logs

If you're encountering problems with the `am2320` collector, follow these steps to retrieve logs and identify potential issues:

- **Run the command** specific to your system (systemd, non-systemd, or Docker container).
- **Examine the output** for any warnings or error messages that might indicate issues.  These messages should provide clues about the root cause of the problem.

#### System with systemd

Use the following command to view logs generated since the last Netdata service restart:

```bash
journalctl _SYSTEMD_INVOCATION_ID="$(systemctl show --value --property=InvocationID netdata)" --namespace=netdata --grep am2320
```

#### System without systemd

Locate the collector log file, typically at `/var/log/netdata/collector.log`, and use `grep` to filter for collector's name:

```bash
grep am2320 /var/log/netdata/collector.log
```

**Note**: This method shows logs from all restarts. Focus on the **latest entries** for troubleshooting current issues.

#### Docker Container

If your Netdata runs in a Docker container named "netdata" (replace if different), use this command:

```bash
docker logs netdata 2>&1 | grep am2320
```


