---
title: Supported chips & development boards
description: Supported chips & development boards
---

import { LinkCard, Steps, Aside, LinkButton } from '@astrojs/starlight/components';

## Supported chips

ESP-Claw requires at least 8MB Flash and 8MB PSRAM.

Currently supported:
- ESP32-S3
- ESP32-P4
- ESP32-C5

## Supported development boards

See [GitHub repository](https://github.com/espressif/esp-claw/tree/master/application/edge_agent/boards).

<Aside title="Need to adapt a new development board?" type="tip">
    ESP-Claw uses ESP Board Manager to support multiple development boards.

    To add other boards, see the [ESP Board Manager component](https://github.com/espressif/esp-gmf/blob/main/packages/esp_board_manager/docs/how_to_customize_board.md),
    and put the board adaptation files in [`application/edge_agent/boards`](https://github.com/espressif/esp-claw/tree/master/application/edge_agent/boards).

    Welcome to submit the board adaptation code to the ESP-Claw repository via Pull Request.
</Aside>
