---
name: Firmware - Bug
about: Report a bug in the Firmware / Embedded development tooling
title: "[Firmware] "
labels: bug, firmware, needs-triage
assignees: ''
---

**Describe the bug**
A clear description of what went wrong.

**MCU / platform affected**
e.g. STM32F4, ESP32, nRF52840, RP2040

**Tool or feature affected**
- [ ] SVD register map loading
- [ ] Datasheet intelligence (PDF parsing)
- [ ] fw_* agent tools
- [ ] Serial monitor
- [ ] Build / flash integration
- [ ] Platform knowledge pack
- [ ] MISRA / CERT-C checks
- [ ] Other

**To reproduce**
Steps to reproduce:
1. 
2. 
3. 

**Expected behavior**
What you expected to happen.

**Actual behavior**
What actually happened. Include any error messages or console output.

**Environment**
- OS:
- NeuralInverse CE version (Help > About):
- Build system (PlatformIO / CMake / ESP-IDF / etc.):
- LLM provider and model used:

**Additional context**
Any other details or screenshots.
