---
feature_ids: [F192, F167]
topics: [harness-eval, eval-a2a, live-verdict]
doc_kind: harness-feedback
feedback_type: live-verdict
domain_id: eval:a2a
packet_id: vhp_eval_a2a_2026_05_23T03_12_57_174Z_eval_F167_2026_05_23_no_finding
source_snapshot: "snapshot:bundle/2026-05-23-eval-a2a-live-verdict/snapshot"
---

# Live Verdict — 2026-05-23-eval-a2a-live-verdict

- Verdict: `keep_observe`
- Phenomenon: No actionable A2A findings: No friction signals detected across 4 components
- Harness: F167/C1 (hold_ball (MCP tool))
- Owner ask: No action required; keep observing the next scheduled eval.
- Re-eval: next eval remains clean at 2026-05-26T03:12:57.174Z

Evidence:
- snapshot:bundle/2026-05-23-eval-a2a-live-verdict/snapshot
- attribution:bundle/2026-05-23-eval-a2a-live-verdict/eval-F167-2026-05-23:no-finding
- metric:c1.zombie_hold_count
- metric:c1.hold_cancel_count
- Checked components: L1, C1, C2, route-serial. Friction metrics examined: c1.zombie_hold_count, c1.hold_cancel_count, c2.verdict_without_pass_count, c2.void_hold_hint_emitted. All values within threshold.

Counterarguments:
- A clean window may hide low-volume failures; keep the scheduled eval active.
