! Synthetic Arista EOS config — fully fictional, for netlog-ai demo only.
!
hostname alpha-sw-02
ip domain-name example.com
ip name-server 10.10.0.10
ip name-server 10.10.0.11
clock timezone UTC
!
no ip routing vrf default
ip routing
!
spanning-tree mode mstp
spanning-tree mst configuration
   name LAB
   revision 1
!
aaa authentication login default local
aaa authorization exec default local
!
username netadmin privilege 15 role network-admin nopassword
username netadmin ssh-key ssh-rsa REDACTED admin@example.com
username readonly privilege 1 role network-operator nopassword
username readonly ssh-key ssh-ed25519 REDACTED audit@example.com
!
management ssh
   no shutdown
!
management api http-commands
   no shutdown
!
ntp server 10.10.0.10 prefer
ntp server 10.10.0.11
!
snmp-server community REDACTED ro 10.10.0.0/24
snmp-server location lab-alpha
snmp-server host 10.10.0.50 version 2c REDACTED
!
logging host 10.10.0.50
logging level all informational
!
vlan 100
   name users
!
vlan 200
   name servers
!
vlan 300
   name iot
!
interface Management1
   ip address 10.10.0.42/24
!
interface Ethernet1
   description uplink to upstream router
   no switchport
   mtu 9214
   ip address 10.10.30.1/30
!
interface Ethernet2
   description leaf user access
   switchport mode access
   switchport access vlan 100
   spanning-tree portfast
!
interface Ethernet3
   description leaf server access
   switchport mode access
   switchport access vlan 200
!
!
vlan 4094
   name MLAG
   trunk group MLAGPEER
!
interface Vlan4094
   description MLAG SVI
   ip address 10.10.250.1/30
!
interface Port-Channel999
   description MLAG-PEER-LINK
   switchport trunk group MLAGPEER
   switchport mode trunk
!
mlag configuration
   domain-id LAB-MLAG
   local-interface Vlan4094
   peer-address 10.10.250.2
   peer-link Port-Channel999
!
router bgp 65020
   router-id 10.10.0.42
   no bgp default ipv4-unicast
   neighbor 10.10.30.6 remote-as 65010
   neighbor 10.10.30.6 description upstream-router
   !
   ! NOTE: no BFD configured — analyzer should flag this
   !
   address-family ipv4
      neighbor 10.10.30.6 activate
!
! NOTE: no LLDP block — analyzer should flag missing LLDP
!
end
