SOURCES
webcam · yolo
mujoco sim
BLACK BOX RUNS
SEALED RECORDINGS · MCAP
NO SIGNAL start the webcam or connect a robot
CAM 01 · LIVE
— FPS — 0 OBJECTS
❯ ⏎ send
BLACK BOX RECORDING
0 events sha-256 · merkle · ed25519
SPATIAL no lidar yet
POINT CLOUD connect a robot with /scan — every return is mapped
through live odometry into the world frame
VERIFIED
director keys `M` record / seal `V` verify `T` tamper one byte `R` runs `C` sources `Esc` clear stamp `?` hide this