# Claude.ai Web Integration

Claude.ai Pro/Max users can add a custom connector to a remote KiCad MCP server.

> **Important**: Claude.ai custom connectors require a **publicly reachable remote MCP endpoint**. They cannot connect to local STDIO servers. For local KiCad access, use Claude Desktop or Claude Code with STDIO transport.

## Requirements

- Claude Pro/Max account
- A publicly hosted KiCad MCP remote server
- (Team/Enterprise) Organization Owner adds connector first

## Setup

1. Go to **Settings → Customize → Connectors → Add custom connector**
2. Enter MCP server URL: `https://mcp.kicad.example.com/mcp`
3. Complete OAuth flow if required

## V1 Tools (Read-only)

- `search_kicad_docs` — documentation search
- `analyze_uploaded_project` — uploaded project zip analysis
- `summarize_project` — project summary
- `explain_drc_report` — DRC interpretation
- `explain_erc_report` — ERC interpretation
- `generate_manufacturing_readiness_report` — readiness report
- `generate_agent_config` — config snippet generation

## Limitations

- No direct local KiCad access
- Project analysis via upload only
- Report generation without local file write
