PT
MCP Control Center
v4
Bridge: offline
● auto-save
Ctrl+Enter Run Ctrl+K Clear ↑↓ History
0 entries
Bridge HTTP
DOWN
port :54321
PT Connection
Offline
not polling
Commands Sent
0
this session
Uptime
00:00
no activity
Connection Health
Offline Bridge Up PT Connected
Poll Activity (last 20)
Bootstrap Snippet

Paste this in PT Extensions → Builder Code Editor and click Run to start the polling loop.

Topology
Template
Routing Protocol
Router Model
Switch Model
Device Counts
Routers: 2
PCs per LAN: 3
Switches per Router: 1
Servers: 0
Options
Enable DHCP
Include WAN (Cloud)
Floating Routes (backup)
Action
—
Sends the complete topology script to Packet Tracer via the live bridge. Make sure PT is connected (Status tab) before building.
Bridge: offline
0 cmds
00:00
PT-MCP Builder Code Editor