# Door Details Catalog - BD Architect Detail Library

**Category:** 05 - Door Details
**Total Files:** 54 .rvt files + 21 preview PNGs
**Source:** `/mnt/d/BDArchitect-DetailLibrary-2025/removed_2026/05 - Door Details/`
**Previews:** `/mnt/d/BDArchitect-DetailLibrary-2025/previews/05 - Door Details/`
**Last Updated:** 2026-03-05

---

## Summary Statistics

| Metric | Count |
|--------|-------|
| Total detail files | 54 |
| Preview images available | 21 |
| Door types covered | 10+ (HM, wood, storefront, elevator, overhead, sliding, bifold, pocket, french, barn, glass, louver) |
| Conditions covered | Head, jamb, sill/threshold, hardware, frame, intermediate |
| Wall systems | Wood frame, steel stud, CMU, concrete, aluminum storefront |

---

## GROUP 1: Hollow Metal (HM) Door Details

### HM Door Head + Jamb (Typical - Steel Stud)
- **File**: DOORS_HEAD+JAMB (TYP).rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Hollow metal
- **Wall System**: Steel stud with GWB
- **Condition**: Head and jamb (combined)
- **Components Used**: HM frame profile, steel stud, GWB layers, sealant
- **Key Elements**: HM frame wrap, anchor clips, GWB return, caulk joint
- **ADA/Code**: Standard commercial frame dimensions
- **Related Details**: DOORS_HEAD+JAMB (WOOD), DOORS_INT H.M. DOOR HEAD_JAMB
- **Drawing Complexity**: Moderate

### HM Door Head + Jamb (Wood Frame)
- **File**: DOORS_HEAD+JAMB (WOOD).rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Hollow metal
- **Wall System**: Wood frame
- **Condition**: Head and jamb (combined)
- **Components Used**: HM frame, wood studs, GWB, shims
- **Key Elements**: HM frame in wood stud wall, blocking, shim space, casing
- **ADA/Code**: Standard residential/light commercial
- **Related Details**: DOORS_HEAD+JAMB (TYP)
- **Drawing Complexity**: Moderate

### Interior HM Door Head/Jamb (Steel Stud)
- **File**: DOORS_INT H.M. DOOR HEAD_JAMB.rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Hollow metal
- **Wall System**: Steel stud with GWB
- **Condition**: Head and jamb
- **Components Used**: HM frame, steel stud framing, GWB, grout fill
- **Key Elements**: Welded HM frame, mortar/grout fill in frame, anchors to studs
- **ADA/Code**: Interior commercial partition
- **Related Details**: DOORS_INT H.M. DOOR HEAD_JAMB (CONC.), DOORS_INT H.M. DOOR HEAD_JAMB (CONCRETE)
- **Drawing Complexity**: Moderate

### Interior HM Door Head/Jamb at Concrete (Version 1)
- **File**: DOORS_INT H.M. DOOR HEAD_JAMB (CONC.).rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Hollow metal
- **Wall System**: Concrete / CMU
- **Condition**: Head and jamb
- **Components Used**: HM frame, concrete/CMU wall, grout fill, anchors
- **Key Elements**: HM frame set in masonry/concrete opening, mortar fill, wire anchors
- **ADA/Code**: Commercial/institutional
- **Related Details**: DOORS_INT H.M. DOOR HEAD_JAMB (CONCRETE)
- **Drawing Complexity**: Moderate

### Interior HM Door Head/Jamb at Concrete (Version 2)
- **File**: DOORS_INT H.M. DOOR HEAD_JAMB (CONCRETE).rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Hollow metal
- **Wall System**: Concrete
- **Condition**: Head and jamb
- **Components Used**: HM frame, cast concrete, anchors, sealant
- **Key Elements**: HM frame in poured concrete wall, expansion anchors
- **ADA/Code**: Commercial/institutional
- **Related Details**: DOORS_INT H.M. DOOR HEAD_JAMB (CONC.)
- **Drawing Complexity**: Moderate

### HM Door Threshold
- **File**: DOOR_H.M._THRESHOLD.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Hollow metal
- **Wall System**: Any
- **Condition**: Sill-threshold
- **Components Used**: Threshold profile, floor finish, sealant, sill pan
- **Key Elements**: Threshold type, weather stripping, floor transition, sealant
- **ADA/Code**: 1/2" max threshold height (ADA), beveled edges
- **Related Details**: DOORS_TYPICAL THRESHOLD, DOOR THRESHOLD AT UNIT ENTRY
- **Drawing Complexity**: Simple

### Exterior HM Door Sill Detail (Preview Available)
- **File**: (preview only - EXT. HM DOOR SILL DETAIL.png)
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Hollow metal (exterior)
- **Wall System**: Steel stud / CMU
- **Condition**: Sill-threshold
- **Components Used**: HM frame sill, threshold, sill pan flashing, concrete slab, sealant
- **Key Elements**: Sill pan flashing with end dams, threshold anchored to slab, weather stripping, floor finish transition at interior, slope to exterior for drainage
- **ADA/Code**: Max 1/2" threshold height, beveled transitions
- **Related Details**: INTERIOR HM DOOR SILL, DOORS_TYPICAL THRESHOLD
- **Drawing Complexity**: Moderate

### Interior HM Door Sill (Preview Available)
- **File**: (preview only - INTERIOR HM DOOR SILL.png)
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Hollow metal (interior)
- **Wall System**: Steel stud
- **Condition**: Sill-threshold
- **Components Used**: HM frame base, floor slab, floor finishes both sides, sealant
- **Key Elements**: Frame base anchored to slab, floor finish transitions (carpet/tile/VCT), minimal threshold or flush condition
- **ADA/Code**: Flush or max 1/4" change without bevel
- **Related Details**: EXT. HM DOOR SILL DETAIL
- **Drawing Complexity**: Simple

### Typical Door Threshold
- **File**: DOORS_TYPICAL THRESHOLD.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: General (HM or wood)
- **Wall System**: Any
- **Condition**: Sill-threshold
- **Components Used**: Standard threshold, floor finish, sealant
- **Key Elements**: Threshold profile, floor finish transition, fasteners
- **ADA/Code**: 1/2" max height exterior, 1/4" max flush interior
- **Related Details**: DOOR_H.M._THRESHOLD, DOOR THRESHOLD AT UNIT ENTRY
- **Drawing Complexity**: Simple

### Door Threshold at Unit Entry
- **File**: DOOR THRESHOLD AT UNIT ENTRY.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: General
- **Wall System**: Steel stud / wood frame
- **Condition**: Sill-threshold
- **Components Used**: Threshold, floor finishes, sealant, fire-rated assembly
- **Key Elements**: Threshold at rated corridor wall, fire seal, floor finish transition between corridor and unit
- **ADA/Code**: ADA compliant threshold, rated corridor condition
- **Related Details**: DOORS_TYPICAL THRESHOLD
- **Drawing Complexity**: Moderate

---

## GROUP 2: Metal Door (Exterior) Details

### Metal Door - Exterior Jamb/Header/Sill
- **File**: METAL DOOR - EXTERIOR JAMB_HEADER_SILL.rvt
- **Type**: Section (3 details combined)
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Metal (exterior)
- **Wall System**: Steel stud with exterior sheathing
- **Condition**: Head, jamb, and sill (all three)
- **Components Used**: Metal frame, weather barrier, flashing, sealant, threshold
- **Key Elements**: Head flashing, jamb sealant, sill pan, weather barrier continuity, drip edge
- **ADA/Code**: Exterior threshold max 1/2", weather sealing required
- **Related Details**: METAL DOOR - INTERIOR JAMB_HEADER
- **Drawing Complexity**: Complex

### Metal Door - Interior Jamb/Header
- **File**: METAL DOOR - INTERIOR JAMB_HEADER.rvt
- **Type**: Section (2 details combined)
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Metal (interior)
- **Wall System**: Steel stud with GWB
- **Condition**: Head and jamb
- **Components Used**: Metal frame, GWB, steel studs, grout fill
- **Key Elements**: Frame anchors, grout fill, GWB return, caulk joint
- **ADA/Code**: Standard interior clearances
- **Related Details**: METAL DOOR - EXTERIOR JAMB_HEADER_SILL
- **Drawing Complexity**: Moderate

---

## GROUP 3: Wood Door Details

### Wood Door Detail (Interior)
- **File**: WOOD DOOR DETAIL (INTERIOR).rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Flush / panel (wood)
- **Wall System**: Wood frame or steel stud
- **Condition**: Head and jamb
- **Components Used**: Wood frame/casing, wood door, GWB, shims
- **Key Elements**: Wood casing profile, shim space, GWB return, stop
- **ADA/Code**: Standard residential/commercial interior
- **Related Details**: WOOD DOOR JAMB, WOOD DOOR HEAD - JAMB SIMILAR
- **Drawing Complexity**: Simple

### Wood Door Jamb
- **File**: WOOD DOOR JAMB.rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Flush / panel (wood)
- **Wall System**: Wood frame
- **Condition**: Jamb
- **Components Used**: Wood jamb, casing, shims, GWB
- **Key Elements**: Jamb profile, casing, stop, shim space, door edge
- **ADA/Code**: Standard residential
- **Related Details**: WOOD DOOR DETAIL (INTERIOR)
- **Drawing Complexity**: Simple

### Wood Door Head + Jamb Similar (Preview Available)
- **File**: (preview only - WOOD DOOR HEAD - JAMB SIMILAR.png)
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Flush / panel (wood)
- **Wall System**: Wood frame with GWB
- **Condition**: Head (jamb similar note)
- **Components Used**: Wood header/jamb frame, wood casing, GWB layers, shims, wood door panel
- **Key Elements**: Wood frame with rabbeted stop, casing trim both sides, GWB to frame, shim space at rough opening, header framing above
- **ADA/Code**: Standard residential clearances
- **Related Details**: WOOD DOOR DETAIL (INTERIOR), WOOD DOOR JAMB
- **Drawing Complexity**: Moderate

---

## GROUP 4: Storefront Door Details

### Storefront Detail at Door Head
- **File**: STORE FRONT_DETAIL @ DOOR HEAD.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Storefront
- **Wall System**: Aluminum storefront system
- **Condition**: Head
- **Components Used**: Aluminum storefront frame, header tube, glass, sealant, flashing
- **Key Elements**: Storefront header extrusion, structural tube above, flashing, glazing gaskets, setting blocks
- **ADA/Code**: Commercial entrance requirements
- **Related Details**: STORE FRONT_DETAIL @ DOOR JAMB, INT. STOREFRONT DOOR HEADER DETAIL
- **Drawing Complexity**: Complex

### Storefront Detail at Door Jamb
- **File**: STORE FRONT_DETAIL @ DOOR JAMB.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Storefront
- **Wall System**: Aluminum storefront system
- **Condition**: Jamb
- **Components Used**: Aluminum storefront jamb, glass, sealant, anchor
- **Key Elements**: Jamb extrusion profile, glass pocket, gaskets, anchor to structure
- **ADA/Code**: Commercial entrance
- **Related Details**: STORE FRONT_DETAIL @ DOOR HEAD
- **Drawing Complexity**: Moderate

### Interior Storefront Door Header Detail (Preview Available)
- **File**: (preview only - INT. STOREFRONT DOOR HEADER DETAIL.png)
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Storefront (interior)
- **Wall System**: Aluminum storefront in steel stud partition
- **Condition**: Head
- **Components Used**: Aluminum storefront header, steel tube support, GWB soffit above, glazing gaskets, door closer mounting
- **Key Elements**: Header extrusion with door closer pocket, steel tube backup, GWB bulkhead/soffit above, glazing channel for sidelite glass, door frame interface
- **ADA/Code**: Interior commercial, closer clearance
- **Related Details**: INT. STOREFRONT DOOR JAMB DETAIL, STORE FRONT_DETAIL @ DOOR HEAD
- **Drawing Complexity**: Complex

### Interior Storefront Door Jamb Detail (Preview Available)
- **File**: (preview only - INT. STOREFRONT DOOR JAMB DETAIL.png)
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Storefront (interior)
- **Wall System**: Aluminum storefront at steel stud
- **Condition**: Jamb
- **Components Used**: Aluminum storefront jamb extrusion, GWB partition, pressure plate, glass
- **Key Elements**: Jamb profile at door leaf, pressure plate glazing, connection to adjacent GWB partition, sealant line
- **ADA/Code**: Interior commercial clearances
- **Related Details**: INT. STOREFRONT DOOR HEADER DETAIL, INT. STOREFRONT JAMB DETAIL @ CONC.
- **Drawing Complexity**: Moderate

### Interior Storefront Jamb at Concrete (Preview Available)
- **File**: (preview only - INT. STOREFRONT JAMB DETAIL @ CONC..png)
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Storefront (interior)
- **Wall System**: Concrete
- **Condition**: Jamb
- **Components Used**: Aluminum storefront jamb, concrete wall, anchor channel, sealant, backer rod
- **Key Elements**: Storefront frame anchored to concrete wall/column, sealant joint between aluminum and concrete, backer rod, continuous gasket
- **ADA/Code**: Interior commercial
- **Related Details**: INT. STOREFRONT DOOR JAMB DETAIL
- **Drawing Complexity**: Moderate

### Exterior Storefront Door Sill - Typical (Preview Available)
- **File**: (preview only - EXT. STOREFRONT DOOR SILL DETAIL - TYPICAL.png)
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Storefront (exterior)
- **Wall System**: Aluminum storefront system
- **Condition**: Sill-threshold
- **Components Used**: Storefront sill extrusion, threshold, concrete slab, waterproofing, sealant, setting blocks
- **Key Elements**: Sill receptor extrusion, ADA-compliant threshold, slab depression for flush condition, waterproofing membrane under sill, weep system, interior floor finish transition
- **ADA/Code**: 1/2" max threshold, beveled, weather sealed
- **Related Details**: EXT. STOREFRONT DOOR SILL DETAIL @ RECESS, EXT. STOREFRONT DOOR SILL DETAIL @ WALK-OFF MAT
- **Drawing Complexity**: Complex

### Exterior Storefront Door Sill at Recess (Preview Available)
- **File**: (preview only - EXT. STOREFRONT DOOR SILL DETAIL @ RECESS.png)
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Storefront (exterior)
- **Wall System**: Aluminum storefront system
- **Condition**: Sill-threshold (recessed entry)
- **Components Used**: Storefront sill, threshold, depressed slab, waterproofing, drain, sealant
- **Key Elements**: Recessed entry slab depression, drainage at recess, threshold at grade change, waterproofing continuity, floor finish transition
- **ADA/Code**: Recessed entry accessibility, max 1/2" threshold, drainage required
- **Related Details**: EXT. STOREFRONT DOOR SILL DETAIL - TYPICAL, EXT. STOREFRONT DOOR SILL DETAIL @ WALK-OFF MAT
- **Drawing Complexity**: Complex

### Exterior Storefront Door Sill at Walk-Off Mat (Preview Available - 4 variants)
- **File**: (preview only - EXT. STOREFRONT DOOR SILL DETAIL @ WALK-OFF MAT.png + .0004/.0005/.0006 variants)
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Storefront (exterior)
- **Wall System**: Aluminum storefront system
- **Condition**: Sill-threshold (walk-off mat)
- **Components Used**: Storefront sill, threshold, recessed walk-off mat frame, concrete slab depression, waterproofing, drain
- **Key Elements**: Walk-off mat recess in slab, mat frame flush with finish floor, drainage under mat, threshold transition, waterproofing membrane continuity. Four variants show different mat frame depths and drainage configurations.
- **ADA/Code**: Flush walk-off mat (no trip hazard), 1/2" max threshold, mat recess flush with adjacent floor
- **Related Details**: EXT. STOREFRONT DOOR SILL DETAIL - TYPICAL, EXT. STOREFRONT DOOR SILL DETAIL @ RECESS
- **Drawing Complexity**: Complex

---

## GROUP 5: Elevator Door Details

### Elevator Door Head/Jamb Detail 1
- **File**: ELEVATOR DOOR HEAD_JAMB DTL 1.rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Elevator
- **Wall System**: Steel stud / CMU
- **Condition**: Head and jamb
- **Components Used**: Elevator entrance frame, wall framing, GWB, grout fill
- **Key Elements**: Elevator entrance assembly, frame anchors, grout-filled frame, fire-rated assembly
- **ADA/Code**: ADA cab dimensions, hall call placement, 80" min clear opening height
- **Related Details**: ELEVATOR DOOR HEAD_JAMB DTL 2, ELEVATOR DOOR HEAD DETAIL
- **Drawing Complexity**: Complex

### Elevator Door Head/Jamb Detail 2
- **File**: ELEVATOR DOOR HEAD_JAMB DTL 2.rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Elevator
- **Wall System**: Steel stud / CMU
- **Condition**: Head and jamb (alternate configuration)
- **Components Used**: Elevator entrance frame, wall framing, cladding, anchors
- **Key Elements**: Alternate frame detail, different anchor pattern, wall finish interface
- **ADA/Code**: Same as DTL 1
- **Related Details**: ELEVATOR DOOR HEAD_JAMB DTL 1
- **Drawing Complexity**: Complex

### Elevator Door Head Detail
- **File**: ELEVATOR DOOR HEAD DETAIL.rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Elevator
- **Wall System**: Steel stud
- **Condition**: Head
- **Components Used**: Elevator header, structural support, fascia, GWB
- **Key Elements**: Header beam/angle, fascia panel, GWB soffit, fire-stopping
- **ADA/Code**: Min 80" clear opening height
- **Related Details**: ELEVATOR DOOR JAMB DETAIL, ELEVATOR DOOR SILL DETAIL
- **Drawing Complexity**: Complex

### Elevator Door Jamb Detail
- **File**: ELEVATOR DOOR JAMB DETAIL.rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Elevator
- **Wall System**: Steel stud
- **Condition**: Jamb
- **Components Used**: Elevator entrance frame jamb, wall framing, GWB, anchors
- **Key Elements**: Entrance jamb profile, wall return, anchor clips, grout fill
- **ADA/Code**: Min 36" clear opening width
- **Related Details**: ELEVATOR DOOR HEAD DETAIL, ELEVATOR DOOR SILL DETAIL
- **Drawing Complexity**: Complex

### Elevator Door Sill Detail
- **File**: ELEVATOR DOOR SILL DETAIL.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Elevator
- **Wall System**: Concrete/steel structure
- **Condition**: Sill-threshold
- **Components Used**: Elevator sill, structural slab, fire-stopping, floor finish
- **Key Elements**: Sill angle, floor finish transition, fire-stopping between shaft and landing, structural support
- **ADA/Code**: Level landing required, max 1-1/4" gap between car and landing sills
- **Related Details**: ELEVATOR DOOR HEAD DETAIL, ELEVATOR DOOR JAMB DETAIL
- **Drawing Complexity**: Complex

### Elevator Jamb Detail (Alternate)
- **File**: ELEVATOR JAMB DETAIL.rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Elevator
- **Wall System**: CMU / concrete
- **Condition**: Jamb
- **Components Used**: Elevator entrance frame, CMU wall, grout, anchors
- **Key Elements**: Frame in masonry wall, grouted cells adjacent to frame, wire anchors
- **ADA/Code**: Standard elevator entrance
- **Related Details**: ELEVATOR DOOR JAMB DETAIL
- **Drawing Complexity**: Moderate

### Elevator Door Jamb (Simple)
- **File**: ELEVATOR_DOOR JAMB.rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Elevator
- **Wall System**: Steel stud
- **Condition**: Jamb
- **Components Used**: Entrance frame, steel stud, GWB
- **Key Elements**: Simplified jamb condition, frame-to-wall interface
- **ADA/Code**: Standard elevator entrance
- **Related Details**: ELEVATOR DOOR JAMB DETAIL, ELEVATOR JAMB DETAIL
- **Drawing Complexity**: Simple

---

## GROUP 6: Overhead / Garage Door Details

### Overhead Coiling Door Jamb Detail
- **File**: OVERHEAD COILING DOOR JAMB DTL.rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Overhead (coiling)
- **Wall System**: CMU / steel frame
- **Condition**: Jamb
- **Components Used**: Guide channel, angle frame, CMU wall, anchor bolts
- **Key Elements**: Coiling door guide channel, structural angle, anchor bolts to masonry, weather seal
- **ADA/Code**: N/A (service/industrial door)
- **Related Details**: OVERHEAD DOOR_HEAD, OVERHEAD DOOR_THRESHOLD
- **Drawing Complexity**: Moderate

### Overhead Door Head
- **File**: OVERHEAD DOOR_HEAD.rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Overhead (sectional or coiling)
- **Wall System**: CMU / steel frame
- **Condition**: Head
- **Components Used**: Lintel/header, guide track, barrel/coil housing, wall framing
- **Key Elements**: Header beam/lintel, track mounting, coil housing above, weather hood/flashing
- **ADA/Code**: N/A (service door)
- **Related Details**: OVERHEAD COILING DOOR JAMB DTL, OVERHEAD DOOR_THRESHOLD
- **Drawing Complexity**: Complex

### Overhead Door Threshold
- **File**: OVERHEAD DOOR_THRESHOLD.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Overhead
- **Wall System**: CMU / concrete
- **Condition**: Sill-threshold
- **Components Used**: Floor slab, threshold angle, weather seal, slab depression
- **Key Elements**: Slab transition, bottom seal, threshold angle embedded in concrete, slope to drain
- **ADA/Code**: N/A (service/vehicle door)
- **Related Details**: OVERHEAD DOOR_HEAD, OVERHEAD COILING DOOR JAMB DTL
- **Drawing Complexity**: Simple

### Garage Door Jamb Detail
- **File**: GARAGE DOOR JAMB DTL.rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Overhead (residential garage)
- **Wall System**: Wood frame / CMU
- **Condition**: Jamb
- **Components Used**: Track bracket, wood/steel jamb, weather stripping, wall framing
- **Key Elements**: Track mounting bracket, jamb trim, weather seal, wall interface
- **ADA/Code**: N/A (residential garage)
- **Related Details**: DOOR_GARAGE_JAMB
- **Drawing Complexity**: Simple

### Garage Door Jamb (Alternate)
- **File**: DOOR_GARAGE_JAMB.rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Overhead (residential garage)
- **Wall System**: Wood frame
- **Condition**: Jamb
- **Components Used**: Track bracket, wood jamb/casing, weather stripping
- **Key Elements**: Alternate jamb treatment, casing profile, weather seal
- **ADA/Code**: N/A (residential garage)
- **Related Details**: GARAGE DOOR JAMB DTL
- **Drawing Complexity**: Simple

---

## GROUP 7: Specialty Door Details (Sliding, Bifold, Pocket, French, Barn)

### Exterior Sliding Door (Preview Available)
- **File**: (preview only - EXTERIOR SLIDING DOOR.png)
- **Type**: Section (head and sill)
- **Scale**: 3" = 1'-0"
- **Door Type**: Sliding (exterior)
- **Wall System**: Wood frame with exterior sheathing
- **Condition**: Head and sill
- **Components Used**: Aluminum sliding door frame, track, rollers, weather stripping, flashing, sill pan, threshold
- **Key Elements**: Head extrusion with weep, track and roller assembly at sill, multi-point weather seal, sill pan with back dam, structural header above, interior/exterior finish transitions. Two section cuts shown (head and sill).
- **ADA/Code**: Max 3/4" exterior threshold (1/2" preferred), operable hardware 48" max
- **Related Details**: NANA DOOR HEAD, NANA DOOR JAMB, EXT. SLIDER WINDOW JAMB DETAIL
- **Drawing Complexity**: Complex

### Exterior Slider Window Jamb Detail (Preview Available)
- **File**: (preview only - EXT. SLIDER WINDOW JAMB DETAIL.png)
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Sliding (exterior, window/door hybrid)
- **Wall System**: Wood frame with exterior cladding
- **Condition**: Jamb
- **Components Used**: Aluminum slider frame, weather barrier, backer rod, sealant, interior/exterior trim
- **Key Elements**: Slider frame in rough opening, weather barrier lapped to frame, sealant joint with backer rod, interior casing, exterior trim/cladding interface
- **ADA/Code**: Operable hardware max 48" AFF
- **Related Details**: EXTERIOR SLIDING DOOR
- **Drawing Complexity**: Moderate

### NanaWall Door Head
- **File**: NANA DOOR HEAD.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Sliding (folding glass wall - NanaWall)
- **Wall System**: Wood frame / steel
- **Condition**: Head
- **Components Used**: NanaWall head track, structural header, flashing, weather seal
- **Key Elements**: Top-hung track system, structural header, head flashing, weather gaskets, glass panel interface
- **ADA/Code**: Max 1/2" threshold at floor
- **Related Details**: NANA DOOR JAMB
- **Drawing Complexity**: Complex

### NanaWall Door Jamb
- **File**: NANA DOOR JAMB.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Sliding (folding glass wall - NanaWall)
- **Wall System**: Wood frame / steel
- **Condition**: Jamb
- **Components Used**: NanaWall jamb extrusion, structural framing, sealant, weather seal
- **Key Elements**: Jamb channel, locking/latching interface, weather seal, structural support at jamb
- **ADA/Code**: Operable hardware requirements
- **Related Details**: NANA DOOR HEAD
- **Drawing Complexity**: Complex

### Head/Sill Bifold Detail
- **File**: HEAD_SILL BIFOLD DETAIL.rvt
- **Type**: Section (head and sill combined)
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Bifold
- **Wall System**: Wood frame
- **Condition**: Head and sill
- **Components Used**: Bifold track, pivot hardware, threshold, header
- **Key Elements**: Top track with pivot bracket, bottom pivot and guide, threshold condition, clearance dimensions
- **ADA/Code**: Closet bifold - no specific ADA for closet doors unless accessible route
- **Related Details**: DOOR DETAIL - BI-FOLD & CLOSET SLIDING
- **Drawing Complexity**: Moderate

### Bifold and Closet Sliding Door Detail (Preview Available)
- **File**: (preview only - DOOR DETAIL - BI-FOLD _ CLOSET SLIDING.png)
- **Type**: Section (head detail)
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Bifold and closet sliding
- **Wall System**: Wood frame
- **Condition**: Head
- **Components Used**: Bifold track header, sliding track, pivot hardware, wood frame, GWB, blocking
- **Key Elements**: Top track mounted to header blocking, bifold pivot bracket, sliding track for bypass doors, adjustable pivot pin, GWB return to track, door panel edge profiles. Shows both bifold and sliding bypass configurations in one detail.
- **ADA/Code**: Accessible closet doors require 32" min clear, hardware max 48" AFF
- **Related Details**: HEAD_SILL BIFOLD DETAIL
- **Drawing Complexity**: Moderate

### Pocket Door Head + Jamb (Preview Available)
- **File**: (preview only - POCKET DOOR HEAD - JAMB.png)
- **Type**: Section (head and jamb combined)
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Pocket
- **Wall System**: Wood frame (thickened for pocket)
- **Condition**: Head and jamb
- **Components Used**: Pocket door frame/track, split studs, steel header track, GWB, trim
- **Key Elements**: Steel track header in wall cavity, split stud framing at pocket, door guide at floor, converging trim at opening, steel channel frame, roller hardware above. Shows track detail at head and split stud pocket at jamb.
- **ADA/Code**: 32" min clear opening, accessible hardware (D-pull, not recessed pull)
- **Related Details**: HEAD_SILL BIFOLD DETAIL
- **Drawing Complexity**: Complex

### French Door
- **File**: FRENCH DOOR.rvt
- **Type**: Section / elevation
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: French
- **Wall System**: Wood frame
- **Condition**: Head, jamb, and mullion
- **Components Used**: French door frame, astragal, weather stripping, glazing
- **Key Elements**: Astragal at meeting stile, glass panel layout, frame profile, weather seal at astragal
- **ADA/Code**: Active leaf min 32" clear
- **Related Details**: ENTRY DOUBLE DOOR, EXTERIOR ALUM. FRENCH DOOR SILL
- **Drawing Complexity**: Moderate

### Exterior Aluminum French Door Sill (Preview Available)
- **File**: (preview only - EXTERIOR ALUM. FRENCH DOOR SILL.png)
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: French (exterior, aluminum)
- **Wall System**: Wood frame with exterior finish
- **Condition**: Sill-threshold
- **Components Used**: Aluminum sill extrusion, sill pan flashing, threshold, weather stripping, floor finish, sealant
- **Key Elements**: Aluminum sill profile with integral weep, sill pan flashing beneath with back dam, weather stripping at door bottom, interior floor finish transition, exterior landing/grade relationship
- **ADA/Code**: Max 1/2" threshold height, bevel required if over 1/4"
- **Related Details**: FRENCH DOOR
- **Drawing Complexity**: Complex

### Entry Double Door
- **File**: ENTRY DOUBLE DOOR.rvt
- **Type**: Section / elevation
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Panel (double entry)
- **Wall System**: Wood frame
- **Condition**: Head, jamb, and mullion
- **Components Used**: Entry door frame, transom bar, sidelite, astragal
- **Key Elements**: Double door astragal, frame profile, weatherstripping, entry threshold
- **ADA/Code**: Active leaf min 32" clear, hardware 34-48" AFF
- **Related Details**: FRENCH DOOR
- **Drawing Complexity**: Moderate

### Barn Door Hardware Section
- **File**: DOOR_BARN DOOR HARDWARE SECTION.rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Barn (sliding)
- **Wall System**: Wood frame / steel stud
- **Condition**: Hardware
- **Components Used**: Barn door track, hangers, door panel, blocking, wall mount
- **Key Elements**: Track rail, roller hanger mechanism, wall blocking for track, door panel, floor guide, clearance from wall
- **ADA/Code**: Hardware max 48" AFF (track typically at 80"+, hardware on face)
- **Related Details**: Copy of DOOR_BARN DOOR HARDWARE
- **Drawing Complexity**: Moderate

### Barn Door Hardware (Copy)
- **File**: Copy of DOOR_BARN DOOR HARDWARE.rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Barn (sliding)
- **Wall System**: Wood frame / steel stud
- **Condition**: Hardware
- **Components Used**: Same as DOOR_BARN DOOR HARDWARE SECTION
- **Key Elements**: Likely a variant or earlier version of barn door hardware detail
- **ADA/Code**: Same as above
- **Related Details**: DOOR_BARN DOOR HARDWARE SECTION
- **Drawing Complexity**: Moderate

---

## GROUP 8: Glass Frame Door Details

### Cascade Glass Door and Sidelite Jamb
- **File**: CASCADE GLASS DOOR & SIDELITE JAMB.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Glass (Cascade series)
- **Wall System**: Aluminum frame system
- **Condition**: Jamb (door + sidelite)
- **Components Used**: Cascade series frame extrusion, glass, gaskets, sealant
- **Key Elements**: Door frame jamb profile, sidelite glazing pocket, meeting condition between door and sidelite, gaskets, structural connection
- **ADA/Code**: Min 32" clear opening for active leaf
- **Related Details**: CASCADE GLASS DOOR HEAD
- **Drawing Complexity**: Complex

### Cascade Glass Door Head
- **File**: CASCADE GLASS DOOR HEAD.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Glass (Cascade series)
- **Wall System**: Aluminum frame system
- **Condition**: Head
- **Components Used**: Cascade series head extrusion, structural backup, glass, gaskets
- **Key Elements**: Head extrusion, closer pocket, glass above door (transom), structural tube
- **ADA/Code**: Min 80" clear height
- **Related Details**: CASCADE GLASS DOOR & SIDELITE JAMB
- **Drawing Complexity**: Complex

### Color Glass Frame Detail - Head
- **File**: COLOR GLASS FRAME DETAIL - HEAD.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Glass (color glass series)
- **Wall System**: Aluminum frame
- **Condition**: Head
- **Components Used**: Colored aluminum frame extrusion, glass, gaskets, structural backup
- **Key Elements**: Head extrusion profile, color finish, glass setting, gaskets
- **ADA/Code**: Standard commercial entrance
- **Related Details**: COLOR GLASS FRAME DETAIL - JAMB, COLOR GLASS FRAME DETAIL - INTERMEDIATE
- **Drawing Complexity**: Moderate

### Color Glass Frame Detail - Intermediate
- **File**: COLOR GLASS FRAME DETAIL - INTERMEDIATE.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Glass (color glass series)
- **Wall System**: Aluminum frame
- **Condition**: Intermediate (horizontal mullion / transom bar)
- **Components Used**: Intermediate horizontal extrusion, glass above/below, gaskets
- **Key Elements**: Transom bar profile, glass setting both sides, gasket system, structural connection
- **ADA/Code**: N/A (intermediate member)
- **Related Details**: COLOR GLASS FRAME DETAIL - HEAD, COLOR GLASS FRAME DETAIL - JAMB
- **Drawing Complexity**: Moderate

### Color Glass Frame Detail - Jamb
- **File**: COLOR GLASS FRAME DETAIL - JAMB.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Glass (color glass series)
- **Wall System**: Aluminum frame
- **Condition**: Jamb
- **Components Used**: Colored aluminum jamb extrusion, glass, gaskets, anchor
- **Key Elements**: Jamb extrusion profile, glass pocket, gaskets, wall anchor
- **ADA/Code**: Standard commercial
- **Related Details**: COLOR GLASS FRAME DETAIL - HEAD, COLOR GLASS FRAME DETAIL - INTERMEDIATE
- **Drawing Complexity**: Moderate

### No Glass Frame Detail - Head
- **File**: NO GLASS FRAME DETAIL - HEAD.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Glass (frame without glass - solid panel option)
- **Wall System**: Aluminum frame
- **Condition**: Head
- **Components Used**: Aluminum frame extrusion, solid panel, gaskets
- **Key Elements**: Head extrusion for solid panel (non-glazed infill), panel setting
- **ADA/Code**: Standard commercial
- **Related Details**: NO GLASS FRAME DETAIL - JAMB, NO GLASS FRAME DETAIL - INTERMEDIATE
- **Drawing Complexity**: Simple

### No Glass Frame Detail - Intermediate
- **File**: NO GLASS FRAME DETAIL - INTERMEDIATE.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Glass (frame without glass - solid panel option)
- **Wall System**: Aluminum frame
- **Condition**: Intermediate
- **Components Used**: Intermediate extrusion, solid panels above/below
- **Key Elements**: Horizontal member for solid panel infill
- **ADA/Code**: N/A
- **Related Details**: NO GLASS FRAME DETAIL - HEAD, NO GLASS FRAME DETAIL - JAMB
- **Drawing Complexity**: Simple

### No Glass Frame Detail - Jamb
- **File**: NO GLASS FRAME DETAIL - JAMB.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Glass (frame without glass - solid panel option)
- **Wall System**: Aluminum frame
- **Condition**: Jamb
- **Components Used**: Aluminum jamb extrusion, solid panel
- **Key Elements**: Jamb extrusion for solid infill panel
- **ADA/Code**: Standard commercial
- **Related Details**: NO GLASS FRAME DETAIL - HEAD, NO GLASS FRAME DETAIL - INTERMEDIATE
- **Drawing Complexity**: Simple

### Sklar Door-Window Details
- **File**: SKLAR DOOR-WINDOW DETAILS.rvt
- **Type**: Section (multiple details)
- **Scale**: 3" = 1'-0"
- **Door Type**: Glass (Sklar series - door/window combination)
- **Wall System**: Aluminum frame
- **Condition**: Multiple (head, jamb, sill, mullion)
- **Components Used**: Sklar series extrusions, glass, gaskets, structural backup
- **Key Elements**: Complete series of details for Sklar door-window system
- **ADA/Code**: Commercial entrance requirements
- **Related Details**: CASCADE, COLOR GLASS series
- **Drawing Complexity**: Complex

### WW 7000 Door Jamb at Hinge Side with Panic Device
- **File**: WW 7000 DETAIL DOOR JAMB @ HINGE SIDE WITH PANIC DEVICE.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Glass (WW 7000 series - commercial)
- **Wall System**: Aluminum frame
- **Condition**: Jamb (hinge side with panic hardware)
- **Components Used**: WW 7000 frame extrusion, panic device, hinge, glass
- **Key Elements**: Hinge pocket, panic device arm clearance, frame profile, glass setting
- **ADA/Code**: Panic hardware for egress (NFPA 101), push-side max 15 lbf
- **Related Details**: WW 7000 DOOR JAMB @ HINGE, WW 7000 DOOR INTERMEDIATE DETAIL, WW 7000 JAMB
- **Drawing Complexity**: Complex

### WW 7000 Door Intermediate Detail
- **File**: WW 7000 DOOR INTERMEDIATE DETAIL.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Glass (WW 7000 series)
- **Wall System**: Aluminum frame
- **Condition**: Intermediate (transom/horizontal mullion)
- **Components Used**: WW 7000 intermediate extrusion, glass, gaskets
- **Key Elements**: Horizontal member profile, glass setting both directions
- **ADA/Code**: N/A
- **Related Details**: WW 7000 DOOR JAMB @ HINGE, WW 7000 JAMB
- **Drawing Complexity**: Moderate

### WW 7000 Door Jamb at Hinge
- **File**: WW 7000 DOOR JAMB @ HINGE.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Glass (WW 7000 series)
- **Wall System**: Aluminum frame
- **Condition**: Jamb (hinge side, no panic device)
- **Components Used**: WW 7000 frame, hinge, glass
- **Key Elements**: Hinge pocket detail, frame profile at hinge leaf
- **ADA/Code**: Standard commercial entrance
- **Related Details**: WW 7000 DETAIL DOOR JAMB @ HINGE SIDE WITH PANIC DEVICE
- **Drawing Complexity**: Moderate

### WW 7000 Jamb
- **File**: WW 7000 JAMB.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Glass (WW 7000 series)
- **Wall System**: Aluminum frame
- **Condition**: Jamb (strike side / general)
- **Components Used**: WW 7000 jamb extrusion, glass, gaskets
- **Key Elements**: Jamb profile, lock/strike pocket, glass setting
- **ADA/Code**: Standard commercial entrance
- **Related Details**: WW 7000 DOOR JAMB @ HINGE
- **Drawing Complexity**: Moderate

---

## GROUP 9: Reference / ADA / Hardware Details

### Door Elevations, Schedule and Hardware (Preview Available)
- **File**: (preview only - DOOR - ELEVATIONS, SCHEDULE AND HARDWARE.png)
- **Type**: Elevation / diagram / schedule
- **Scale**: Various (1/4" = 1'-0" elevations)
- **Door Type**: Multiple (flush, panel, glass, pairs)
- **Wall System**: N/A (reference sheet)
- **Condition**: N/A (reference)
- **Components Used**: Door elevation symbols, schedule table, hardware notations
- **Key Elements**: Standard door elevation types (single, pair, with sidelite, with transom), door schedule format, hardware set references, door type designations. Serves as a reference sheet for door types and hardware groups.
- **ADA/Code**: Hardware heights noted, lever handles required for ADA
- **Related Details**: DOOR HARDWARE LOCATIONS, Maneuvering Clearances at Door1
- **Drawing Complexity**: Moderate (reference/diagram)

### Door Hardware Locations (Preview Available)
- **File**: (preview only - DOOR HARDWARE LOCATIONS.png)
- **Type**: Diagram / elevation
- **Scale**: 1/2" = 1'-0" or NTS
- **Door Type**: General (all types)
- **Wall System**: N/A (reference)
- **Condition**: Hardware
- **Components Used**: Door elevation with hardware location dimensions
- **Key Elements**: Dimension heights for: strike plate, lockset/lever (36" typical), closer, kick plate, threshold. Shows hardware zone diagram with AFF dimensions for all hardware items.
- **ADA/Code**: Lever hardware 34"-48" AFF, closers per ANSI/BHMA, vision lite min 43" to bottom
- **Related Details**: DOOR - ELEVATIONS, SCHEDULE AND HARDWARE, Maneuvering Clearances at Door1
- **Drawing Complexity**: Simple (diagram)

### Door Opening Location
- **File**: DOOR OPENING LOCATION.rvt
- **Type**: Plan / diagram
- **Scale**: 1/4" = 1'-0" or NTS
- **Door Type**: General
- **Wall System**: Any
- **Condition**: N/A (reference for placement)
- **Components Used**: Plan symbols, dimension lines
- **Key Elements**: Shows standard door opening location conventions in plan view - how to dimension door openings from walls/corners
- **ADA/Code**: Min 32" clear opening, maneuvering clearances
- **Related Details**: Maneuvering Clearances at Door1
- **Drawing Complexity**: Simple (diagram)

### Maneuvering Clearances at Door (Preview Available)
- **File**: (preview only - Maneuvering Clearances at Door1.png)
- **Type**: Plan / diagram
- **Scale**: NTS
- **Door Type**: General (all types)
- **Wall System**: Any
- **Condition**: N/A (ADA reference)
- **Components Used**: Plan diagrams with dimension annotations, wheelchair clearance zones
- **Key Elements**: ADA/ICC A117.1 maneuvering clearances at doors. Shows push-side and pull-side clearances for front approach, hinge approach, and latch approach. Dimensions include 60" pull side, 48" push side, 18" latch-side clearance. Multiple approach configurations shown with required floor areas.
- **ADA/Code**: ICC A117.1 / ADA 404.2.4 maneuvering clearances - critical reference
- **Related Details**: DOOR HARDWARE LOCATIONS, DOOR OPENING LOCATION
- **Drawing Complexity**: Moderate (multiple plan diagrams)

### Door Jamb Detail (Preview Available)
- **File**: (preview only - DOOR JAMB DETAIL.png)
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: General (wood or HM)
- **Wall System**: Wood frame with GWB
- **Condition**: Jamb
- **Components Used**: Door frame/jamb, GWB layers, wood stud, insulation, casing, shims
- **Key Elements**: Complete jamb section showing rough opening to finish - wood stud wall with GWB both sides, jamb with rabbet for door stop, shim space, casing trim, insulation in cavity. Detailed annotations for each component.
- **ADA/Code**: Standard residential/commercial clearances
- **Related Details**: WOOD DOOR JAMB, DOORS_HEAD+JAMB (WOOD)
- **Drawing Complexity**: Moderate

---

## GROUP 10: Louver and Access Panel Details

### Louver Jamb Detail
- **File**: LOUVER JAMB DETAIL.rvt
- **Type**: Section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Louver (mechanical)
- **Wall System**: CMU / steel stud
- **Condition**: Jamb
- **Components Used**: Louver frame, wall framing, sealant, anchor
- **Key Elements**: Louver frame profile, blade angle reference, frame-to-wall interface, weather seal
- **ADA/Code**: N/A (mechanical louver)
- **Related Details**: N/A
- **Drawing Complexity**: Simple

### Concealed Frame Flush Access Panel
- **File**: CONCEALED FRAME FLUSH ACCESS PANEL.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: Access panel (flush)
- **Wall System**: GWB on steel stud
- **Condition**: Frame (all around)
- **Components Used**: Concealed frame, flush panel, GWB, spring/cam latch
- **Key Elements**: Concealed hinge, flush panel face (GWB-clad or painted), spring latch, frame anchored to studs
- **ADA/Code**: N/A (access panel, not passage door)
- **Related Details**: N/A
- **Drawing Complexity**: Simple

---

## GROUP 11: Tile / Flooring Transition Details

### Carpet/Tile Transition
- **File**: CARPET_TILE TRANSITION.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: N/A (floor transition at doorway)
- **Wall System**: Any
- **Condition**: N/A (floor transition)
- **Components Used**: Transition strip, carpet, tile, thin-set, subfloor
- **Key Elements**: Transition strip profile, carpet tack strip, tile edge, height difference management
- **ADA/Code**: Max 1/4" level change without bevel, 1/2" with bevel
- **Related Details**: TILE_CARPET TRANSITION
- **Drawing Complexity**: Simple

### Tile/Carpet Transition
- **File**: TILE_CARPET TRANSITION.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: N/A (floor transition at doorway)
- **Wall System**: Any
- **Condition**: N/A (floor transition)
- **Components Used**: Transition strip, tile, carpet, subfloor
- **Key Elements**: Similar to CARPET_TILE TRANSITION - alternate configuration or direction
- **ADA/Code**: Max 1/4" level change without bevel
- **Related Details**: CARPET_TILE TRANSITION
- **Drawing Complexity**: Simple

### Corner Tile Detail
- **File**: CORNER TILE DETAIL.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: N/A (tile detail near door frame)
- **Wall System**: Any
- **Condition**: N/A (tile corner)
- **Components Used**: Tile, thin-set, corner bead/trim, substrate
- **Key Elements**: Outside corner tile condition, corner trim profile, tile edge treatment
- **ADA/Code**: N/A
- **Related Details**: TILE CORNER DETAIL, MIDDLE TILE DETAIL
- **Drawing Complexity**: Simple

### Tile Corner Detail
- **File**: TILE CORNER DETAIL.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: N/A (tile detail)
- **Wall System**: Any
- **Condition**: N/A (tile corner)
- **Components Used**: Tile, thin-set, corner profile, substrate
- **Key Elements**: Inside/outside corner tile treatment
- **ADA/Code**: N/A
- **Related Details**: CORNER TILE DETAIL, MIDDLE TILE DETAIL
- **Drawing Complexity**: Simple

### Middle Tile Detail
- **File**: MIDDLE TILE DETAIL.rvt
- **Type**: Section
- **Scale**: 3" = 1'-0"
- **Door Type**: N/A (tile detail)
- **Wall System**: Any
- **Condition**: N/A (tile field)
- **Components Used**: Tile, thin-set, substrate, backer board
- **Key Elements**: Field tile installation section, substrate preparation, thin-set bed
- **ADA/Code**: N/A
- **Related Details**: CORNER TILE DETAIL, TILE CORNER DETAIL
- **Drawing Complexity**: Simple

### Single Door at Typical Office Entry Condition
- **File**: SINGLE DOOR @ TYP. OFFICE ENTRY CONDITION.rvt
- **Type**: Plan / section
- **Scale**: 1-1/2" = 1'-0"
- **Door Type**: Flush (office entry)
- **Wall System**: Steel stud with GWB
- **Condition**: Frame and threshold at office entry
- **Components Used**: HM or wood frame, GWB partition, sidelite (optional), flooring transition
- **Key Elements**: Typical office entry condition showing door frame in partition, possible sidelite, floor transition at threshold, hardware location
- **ADA/Code**: 32" min clear, maneuvering clearances per ICC A117.1
- **Related Details**: DOOR OPENING LOCATION, Maneuvering Clearances at Door1
- **Drawing Complexity**: Moderate

---

## Cross-Reference Index

### By Condition

| Condition | Files |
|-----------|-------|
| **Head** | DOORS_HEAD+JAMB (TYP), DOORS_HEAD+JAMB (WOOD), DOORS_INT H.M. DOOR HEAD_JAMB (3 variants), ELEVATOR DOOR HEAD DETAIL, ELEVATOR DOOR HEAD_JAMB DTL 1/2, OVERHEAD DOOR_HEAD, CASCADE GLASS DOOR HEAD, COLOR GLASS FRAME DETAIL - HEAD, NO GLASS FRAME DETAIL - HEAD, NANA DOOR HEAD, STORE FRONT_DETAIL @ DOOR HEAD, HEAD_SILL BIFOLD DETAIL |
| **Jamb** | DOORS_HEAD+JAMB (TYP/WOOD), DOORS_INT H.M. (3 variants), ELEVATOR DOOR JAMB DETAIL, ELEVATOR JAMB DETAIL, ELEVATOR_DOOR JAMB, GARAGE DOOR JAMB DTL, DOOR_GARAGE_JAMB, OVERHEAD COILING DOOR JAMB DTL, CASCADE GLASS DOOR & SIDELITE JAMB, COLOR GLASS FRAME DETAIL - JAMB, NO GLASS FRAME DETAIL - JAMB, NANA DOOR JAMB, STORE FRONT_DETAIL @ DOOR JAMB, LOUVER JAMB DETAIL, WW 7000 (4 variants), WOOD DOOR JAMB |
| **Sill/Threshold** | DOOR_H.M._THRESHOLD, DOORS_TYPICAL THRESHOLD, DOOR THRESHOLD AT UNIT ENTRY, ELEVATOR DOOR SILL DETAIL, OVERHEAD DOOR_THRESHOLD, HEAD_SILL BIFOLD DETAIL |
| **Hardware** | DOOR_BARN DOOR HARDWARE SECTION, Copy of DOOR_BARN DOOR HARDWARE, WW 7000 DETAIL DOOR JAMB @ HINGE SIDE WITH PANIC DEVICE |
| **Intermediate** | COLOR GLASS FRAME DETAIL - INTERMEDIATE, NO GLASS FRAME DETAIL - INTERMEDIATE, WW 7000 DOOR INTERMEDIATE DETAIL |

### By Wall System

| Wall System | Files |
|-------------|-------|
| **Wood frame** | DOORS_HEAD+JAMB (WOOD), WOOD DOOR DETAIL (INTERIOR), WOOD DOOR JAMB, HEAD_SILL BIFOLD DETAIL, FRENCH DOOR, ENTRY DOUBLE DOOR, DOOR_BARN DOOR HARDWARE SECTION, GARAGE DOOR JAMB DTL, DOOR_GARAGE_JAMB, NANA DOOR HEAD/JAMB |
| **Steel stud** | DOORS_HEAD+JAMB (TYP), DOORS_INT H.M. DOOR HEAD_JAMB, METAL DOOR - INTERIOR JAMB_HEADER, METAL DOOR - EXTERIOR JAMB_HEADER_SILL, ELEVATOR DOOR HEAD DETAIL, ELEVATOR DOOR JAMB DETAIL, ELEVATOR_DOOR JAMB, SINGLE DOOR @ TYP. OFFICE ENTRY CONDITION |
| **CMU / Concrete** | DOORS_INT H.M. DOOR HEAD_JAMB (CONC.), DOORS_INT H.M. DOOR HEAD_JAMB (CONCRETE), ELEVATOR JAMB DETAIL, OVERHEAD COILING DOOR JAMB DTL, LOUVER JAMB DETAIL |
| **Aluminum storefront** | STORE FRONT (2), CASCADE GLASS (2), COLOR GLASS FRAME (3), NO GLASS FRAME (3), WW 7000 (4), SKLAR DOOR-WINDOW DETAILS |

### By Door Type

| Door Type | Count | Files |
|-----------|-------|-------|
| **Hollow metal** | 9 | DOORS_HEAD+JAMB (2), DOORS_INT H.M. (3), DOOR_H.M._THRESHOLD, DOORS_TYPICAL THRESHOLD, METAL DOOR (2) |
| **Wood** | 3 | WOOD DOOR DETAIL (INTERIOR), WOOD DOOR JAMB, (preview: WOOD DOOR HEAD - JAMB SIMILAR) |
| **Elevator** | 7 | ELEVATOR DOOR HEAD_JAMB DTL 1/2, ELEVATOR DOOR HEAD/JAMB/SILL DETAIL, ELEVATOR JAMB DETAIL, ELEVATOR_DOOR JAMB |
| **Storefront** | 2+previews | STORE FRONT_DETAIL (2), + 7 preview-only variants |
| **Glass frame** | 11 | CASCADE (2), COLOR GLASS FRAME (3), NO GLASS FRAME (3), WW 7000 (4) |
| **Overhead/Garage** | 5 | OVERHEAD COILING DOOR JAMB DTL, OVERHEAD DOOR_HEAD/THRESHOLD, GARAGE DOOR JAMB DTL, DOOR_GARAGE_JAMB |
| **Sliding/NanaWall** | 2+previews | NANA DOOR HEAD/JAMB, + preview: EXTERIOR SLIDING DOOR, EXT. SLIDER WINDOW JAMB |
| **Bifold** | 1+preview | HEAD_SILL BIFOLD DETAIL, + preview: DOOR DETAIL - BI-FOLD & CLOSET SLIDING |
| **Pocket** | preview only | POCKET DOOR HEAD - JAMB |
| **French** | 1+preview | FRENCH DOOR, + preview: EXTERIOR ALUM. FRENCH DOOR SILL |
| **Barn** | 2 | DOOR_BARN DOOR HARDWARE SECTION, Copy of DOOR_BARN DOOR HARDWARE |
| **Louver** | 1 | LOUVER JAMB DETAIL |
| **Access panel** | 1 | CONCEALED FRAME FLUSH ACCESS PANEL |

---

## Preview-Only Details (no .rvt file in removed_2026)

These 21 preview PNGs exist but some correspond to .rvt files not in the `removed_2026` folder (likely still active in the library or from a different source project):

| Preview | Has .rvt in removed_2026? |
|---------|--------------------------|
| DOOR - ELEVATIONS, SCHEDULE AND HARDWARE.png | No |
| DOOR DETAIL - BI-FOLD _ CLOSET SLIDING.png | No (HEAD_SILL BIFOLD DETAIL.rvt is related) |
| DOOR HARDWARE LOCATIONS.png | No |
| DOOR JAMB DETAIL.png | No |
| EXT. HM DOOR SILL DETAIL.png | No |
| EXT. SLIDER WINDOW JAMB DETAIL.png | No |
| EXT. STOREFRONT DOOR SILL DETAIL - TYPICAL.png | No |
| EXT. STOREFRONT DOOR SILL DETAIL @ RECESS.png | No |
| EXT. STOREFRONT DOOR SILL DETAIL @ WALK-OFF MAT (4 variants).png | No |
| EXTERIOR ALUM. FRENCH DOOR SILL.png | No |
| EXTERIOR SLIDING DOOR.png | No |
| INT. STOREFRONT DOOR HEADER DETAIL.png | No |
| INT. STOREFRONT DOOR JAMB DETAIL.png | No |
| INT. STOREFRONT JAMB DETAIL @ CONC..png | No |
| INTERIOR HM DOOR SILL.png | No |
| Maneuvering Clearances at Door1.png | No |
| POCKET DOOR HEAD - JAMB.png | No |
| WOOD DOOR HEAD - JAMB SIMILAR.png | No |

---

## Notes for AI Detail Drawing

### Drawing Priority (most commonly needed)
1. **HM door head/jamb** - every commercial project
2. **Wood door head/jamb** - every residential project
3. **Storefront door sill** - every commercial entrance
4. **Threshold details** - every project (ADA compliance)
5. **Elevator entrance** - any multi-story project
6. **Overhead door** - industrial, commercial, residential garage

### ADA Critical Dimensions
- Door clear opening: 32" min (34" nominal door in 36" frame)
- Threshold height: 1/2" max exterior, 1/4" max interior (without bevel)
- Hardware height: 34" - 48" AFF
- Maneuvering clearances: 60" pull side, 48" push side (front approach)
- Closer force: 5 lbf max (interior), 8.5 lbf max (exterior fire door)
- Vision lite: bottom at 43" max AFF

### Component Library Gaps
The BD Architect library has strong coverage of:
- Commercial HM door conditions (head, jamb, threshold)
- Glass/storefront systems (multiple manufacturers)
- Elevator entrance details

Weaker coverage of:
- Fire-rated door assemblies (label locations, smoke seals)
- Acoustic door details (STC-rated)
- Automatic door operator details
- Revolving door details
- Security door/frame details (detention, blast)
