# Miscellaneous Details Catalog -- BD Architect Detail Library

> Source: `/mnt/d/BDArchitect-DetailLibrary-2025/removed_2026/`
> Generated: 2026-03-05
> Total Files: 98 .rvt files across 8 categories
> Preview Coverage: 04-Floor (13), 07-Stair (1), 14-MEP (5), 15-Typical (6), 99-General (34). No previews for 17-Structural, 18-Fire Protection, 19-Site.

---

## 1. FLOOR DETAILS (14 files)

### Sub-group: Shower & Wet Area

#### SHOWER THRESHOLD DETAIL AT ACCESSIBLE SHOWER WITH 3" SLAB DEPRESSION
- **File**: `SHOWER_THRESHOLD DETAIL AT ACCESSIBLE SHOWER WITH 3_ SLAB DEPRESSION.rvt`
- **Category**: Floor
- **Type**: section
- **Scale**: 1" = 1'-0" (typical)
- **Components Used**: Concrete slab, waterproofing membrane, mortar bed, tile, threshold, drain body
- **Key Elements**: Depressed slab at accessible shower entry; shows 3" depression with sloped mortar bed, waterproofing turn-up at curb, flush transition at threshold for wheelchair access
- **Code/Standards**: ADA/ABA (Section 608 -- shower compartments), IBC Section 1109, ANSI A117.1
- **Related Details**: Ceramic Tile at Shower (preview), Floor Transition Details
- **Drawing Complexity**: moderate

### Sub-group: Expansion Joints

#### EXPANSION JOINT SLAB TO SLAB DTL
- **File**: `EXPANSION JOINT SLAB TO SLAB DTL.rvt`
- **Category**: Floor
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Concrete slab, expansion joint cover assembly, compressible filler, sealant, rebar dowels
- **Key Elements**: Expansion joint between two concrete slabs; shows joint width, cover plate, compressible fill material, sealant bead
- **Code/Standards**: IBC Chapter 19 (concrete), ACI 318
- **Related Details**: Expansion Joint at Terrace
- **Drawing Complexity**: simple

#### EXPANSION JOINT AT TERRACE
- **File**: `EXPANSION JOINT AT TERRACE.rvt`
- **Category**: Floor
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Concrete slab, expansion joint assembly, waterproofing membrane, pavers/topping, compressible filler
- **Key Elements**: Expansion joint at exterior terrace condition; shows waterproofing continuity through joint, drainage provision, surface cover plate
- **Code/Standards**: IBC Chapter 19, ASTM C920 (sealants)
- **Related Details**: Expansion Joint Slab to Slab DTL, Terrace Edge DTL
- **Drawing Complexity**: moderate

### Sub-group: Terrace & Planter

#### TERRACE DRAIN DTL
- **File**: `TERRACE DRAIN DTL.rvt`
- **Category**: Floor
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Concrete slab, waterproofing membrane, protection board, drainage mat, mortar bed, pavers/tile, drain body with clamping ring
- **Key Elements**: Floor drain assembly at terrace; shows clamping ring at waterproofing layer, slope to drain, topping slab buildup
- **Code/Standards**: IBC Chapter 15 (roofs), IPC (plumbing drainage)
- **Related Details**: Planter Floor Drain Terrace Detail, Terrace Edge DTL
- **Drawing Complexity**: moderate

#### PLANTER FLOOR DRAIN TERRACE DETAIL
- **File**: `PLANTER FLOOR DRAIN TERRACE DETAIL.rvt`
- **Category**: Floor
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Concrete slab, waterproofing membrane, drainage mat, filter fabric, planter soil, drain body, overflow pipe
- **Key Elements**: Drain at planter within terrace assembly; shows soil containment, root barrier, drainage layer, overflow provisions
- **Code/Standards**: IBC Chapter 15, local landscape/drainage codes
- **Related Details**: Terrace Planter @ Balcony, Terrace Planter @ Courtyard
- **Drawing Complexity**: moderate

#### TERRACE EDGE DTL
- **File**: `TERRACE EDGE DTL.rvt`
- **Category**: Floor
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Concrete slab, waterproofing membrane, metal edge flashing, pavers, mortar bed, drip edge
- **Key Elements**: Edge termination of terrace assembly; shows waterproofing turn-down at edge, drip edge profile, fascia treatment
- **Code/Standards**: IBC Chapter 15, SMACNA (sheet metal)
- **Related Details**: Terrace Drain DTL, Flush Curb Detail
- **Drawing Complexity**: simple

#### TERRACE PLANTER @ BALCONY
- **File**: `TERRACE PLANTER @ BALCONY.rvt`
- **Category**: Floor
- **Type**: section
- **Scale**: 1" = 1'-0"
- **Components Used**: Concrete slab, waterproofing membrane, planter curb, drainage layer, filter fabric, soil, vegetation
- **Key Elements**: Built-in planter at balcony edge; shows curb height, waterproofing containment, drainage provisions, railing attachment above
- **Code/Standards**: IBC Chapter 15, structural loading per ASCE 7
- **Related Details**: Terrace Planter @ Courtyard, Planter Floor Drain Terrace Detail
- **Drawing Complexity**: moderate

#### TERRACE PLANTER @ COURTYARD
- **File**: `TERRACE PLANTER @ COURTYARD.rvt`
- **Category**: Floor
- **Type**: section
- **Scale**: 1" = 1'-0"
- **Components Used**: Concrete slab, waterproofing membrane, planter walls (CMU or concrete), drainage gravel, filter fabric, soil
- **Key Elements**: Ground-level courtyard planter; shows foundation/footing, waterproofing below grade, drainage layer, overflow to storm system
- **Code/Standards**: IBC Chapter 15, local landscape codes
- **Related Details**: Terrace Planter @ Balcony
- **Drawing Complexity**: moderate

### Sub-group: Floor Transitions

#### FLOOR TRANSITION DETAILS
- **File**: `FLOOR TRANSITION DETAILS.rvt`
- **Category**: Floor
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Concrete slab, tile, carpet, transition strip (metal), mortar bed, self-leveling underlayment
- **Key Elements**: Transition between different floor finishes (tile-to-carpet, tile-to-tile at height change); shows reducer strips, ADA-compliant slope transitions
- **Code/Standards**: ADA/ABA (1/4" vertical, 1/2" beveled max), IBC 1003.4
- **Related Details**: Flooring Transitions, Flush Curb Detail
- **Drawing Complexity**: simple

#### FLOORING TRANSITIONS
- **File**: `FLOORING TRANSITIONS.rvt`
- **Category**: Floor
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Concrete slab, various finish flooring, metal transition strips, mortar bed, adhesive
- **Key Elements**: Multiple floor-to-floor transition conditions; flush and ramped transitions between different materials and heights
- **Code/Standards**: ADA/ABA, IBC 1003.4
- **Related Details**: Floor Transition Details
- **Drawing Complexity**: simple

### Sub-group: Curbs & Penetrations

#### FLUSH CURB DETAIL - INTERIOR TO SUNSET DECK
- **File**: `FLUSH CURB DETAIL - INTERIOR TO SUNSET DECK.rvt`
- **Category**: Floor
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Concrete slab, waterproofing membrane, mortar bed, tile/pavers, door threshold, sealant
- **Key Elements**: Flush threshold between interior floor and exterior deck; shows waterproofing turn-up, recessed slab at exterior, drainage channel at threshold
- **Code/Standards**: ADA (accessible threshold), IBC Chapter 15 (waterproofing)
- **Related Details**: Floor Transition Details, Terrace Edge DTL
- **Drawing Complexity**: moderate

#### PRE-FABRICATED METAL CURB
- **File**: `PRE-FABRICATED METAL CURB.rvt`
- **Category**: Floor
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Galvanized steel curb, concrete slab, waterproofing membrane, sealant, fasteners
- **Key Elements**: Pre-fab metal curb at slab edge or equipment base; shows anchorage to slab, flashing integration, sealant joints
- **Code/Standards**: SMACNA, IBC Chapter 15
- **Related Details**: Flush Curb Detail
- **Drawing Complexity**: simple

#### ENCLOSURE FOR MULTIPLE PIPING THRU DECK
- **File**: `ENCLOSURE FOR MULTIPLE PIPING THRU DECK.rvt`
- **Category**: Floor
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Concrete slab, pipe sleeve, fire caulk, waterproofing membrane, metal enclosure/curb, sealant
- **Key Elements**: Multiple pipe penetrations through elevated deck slab; shows fire-rated enclosure, waterproofing continuity, curb height above finished floor
- **Code/Standards**: IBC Section 714 (penetrations), NFPA 101, UL firestop systems
- **Related Details**: WW 7000 Detail @ Slab
- **Drawing Complexity**: moderate

#### WW 7000 DETAIL @ SLAB
- **File**: `WW 7000 DETAIL @ SLAB.rvt`
- **Category**: Floor
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Concrete slab, WW 7000 waterstop system, rebar, formwork
- **Key Elements**: Waterstop installation at concrete construction joint in slab; shows waterstop profile embedded in pour, rebar clearance
- **Code/Standards**: ACI 318, ACI 350 (water-retaining structures)
- **Related Details**: Expansion Joint Slab to Slab DTL
- **Drawing Complexity**: simple

---

## 2. STAIR & RAILING DETAILS (27 files)

### Sub-group: Railing -- Balcony

#### BALCONY RAILING DETAIL
- **File**: `BALCONY RAILING DETAIL.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Steel post, top rail, intermediate rail/pickets, base plate, concrete slab, waterproofing membrane, anchor bolts
- **Key Elements**: Railing attachment to balcony slab edge; shows base plate anchorage, post spacing, rail heights, waterproofing flashing at base
- **Code/Standards**: IBC 1015 (guards), 42" min height residential/commercial, 200 lb concentrated load
- **Related Details**: Railing Detail @ Balcony, Balcony Unit Railing Detail W/Glass
- **Drawing Complexity**: moderate

#### BALCONY UNIT RAILING DETAIL W/GLASS
- **File**: `BALCONY UNIT RAILING DETAIL W_GLASS.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Steel post, top rail, glass panel (tempered/laminated), glass clamp/shoe, base plate, concrete slab
- **Key Elements**: Glass panel railing system at unit balcony; shows glass shoe channel, glass panel thickness, top cap rail, post-to-slab connection
- **Code/Standards**: IBC 1015, ASTM C1048 (tempered glass), 16 CFR 1201 (safety glazing)
- **Related Details**: Balcony Railing Detail, Enlarged Section & Railing Detail @ Typ Unit Balcony
- **Drawing Complexity**: complex

#### ENLARGED SECTION & RAILING DETAIL @ TYP UNIT BALCONY
- **File**: `ENLARGED SECTION & RAILING DETAIL @ TYP UNIT BALCONY.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1" = 1'-0"
- **Components Used**: Steel post, top rail, pickets/glass, base plate, concrete slab, waterproofing, exterior wall assembly, sliding door sill
- **Key Elements**: Combined wall section and railing detail at typical unit balcony; shows full assembly from interior floor through exterior wall to railing, slab edge, waterproofing turn-up
- **Code/Standards**: IBC 1015, IBC Chapter 14 (exterior walls)
- **Related Details**: Balcony Railing Detail, Balcony Unit Railing Detail W/Glass
- **Drawing Complexity**: complex

#### RAILING DETAIL @ BALCONY
- **File**: `RAILING DETAIL @ BALCONY.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Steel post, top rail, balusters/pickets, base plate, concrete slab edge, anchor bolts
- **Key Elements**: Standard balcony railing with pickets; shows 4" max picket spacing, rail heights, base plate detail at slab edge
- **Code/Standards**: IBC 1015, 4" sphere rule (1015.4)
- **Related Details**: Railing Detail @ Balcony Copy 1, Balcony Railing Detail
- **Drawing Complexity**: moderate

#### RAILING DETAIL @ BALCONY COPY 1
- **File**: `RAILING DETAIL @ BALCONY Copy 1.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Steel post, top rail, balusters/pickets, base plate, concrete slab
- **Key Elements**: Alternate balcony railing configuration; variant of standard railing detail with different post/picket arrangement
- **Code/Standards**: IBC 1015
- **Related Details**: Railing Detail @ Balcony
- **Drawing Complexity**: moderate

### Sub-group: Railing -- Terrace & Amenity

#### RAILING DETAIL @ AMENITY PLANTERS
- **File**: `RAILING DETAIL @ AMENITY PLANTERS.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Steel post, top rail, pickets, planter curb (concrete/masonry), waterproofing, anchor bolts
- **Key Elements**: Railing mounted on top of planter curb at amenity area; shows post anchorage through planter wall, guard height measured from walking surface
- **Code/Standards**: IBC 1015, guard height requirements from adjacent walking surface
- **Related Details**: Railing Detail @ Amenity Terrace
- **Drawing Complexity**: moderate

#### RAILING DETAIL @ AMENITY TERRACE
- **File**: `RAILING DETAIL @ AMENITY TERRACE.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Steel post, top rail, pickets or cable rail, base plate, terrace slab, waterproofing membrane
- **Key Elements**: Railing at amenity deck/terrace edge; shows slab edge condition, waterproofing at post penetration, guard height
- **Code/Standards**: IBC 1015
- **Related Details**: Railing Detail @ Amenity Planters, Pool Deck Railing Detail
- **Drawing Complexity**: moderate

#### POOL DECK RAILING DETAIL
- **File**: `POOL DECK RAILING DETAIL.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Steel/aluminum post, top rail, glass panel or pickets, base plate, pool deck slab, waterproofing
- **Key Elements**: Guard railing at pool deck perimeter; shows corrosion-resistant materials, base plate at deck, height compliance
- **Code/Standards**: IBC 1015, local pool barrier codes (IBC 3109), Florida Building Code pool enclosures
- **Related Details**: Pool Deck Railing Detail - 5
- **Drawing Complexity**: moderate

#### POOL DECK RAILING DETAIL - 5
- **File**: `POOL DECK RAILING DETAIL - 5.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Steel/aluminum post, top rail, pickets, base plate, pool deck slab
- **Key Elements**: Variant pool deck railing; alternate configuration (possibly different pool edge condition or material)
- **Code/Standards**: IBC 1015, IBC 3109
- **Related Details**: Pool Deck Railing Detail
- **Drawing Complexity**: moderate

#### GLASS GUARD/BAFFLE
- **File**: `GLASS GUARD_BAFFLE.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Tempered/laminated glass panel, aluminum shoe/channel, top cap, steel post (if any), base anchorage
- **Key Elements**: Glass guard or wind baffle panel; shows glass thickness, shoe channel embedment, silicone setting blocks, top cap rail
- **Code/Standards**: IBC 1015, ASTM C1048, 16 CFR 1201
- **Related Details**: Balcony Unit Railing Detail W/Glass
- **Drawing Complexity**: moderate

### Sub-group: Railing -- ADA Ramp

#### SECTION @ ADA RAMP
- **File**: `SECTION @ ADA RAMP.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1/2" = 1'-0"
- **Components Used**: Concrete ramp slab, handrails (wall-mounted and freestanding), curb/edge protection, landing slab, rebar
- **Key Elements**: Cross-section through ADA-compliant ramp; shows 1:12 max slope, 36" min clear width, handrail heights (34"-38"), edge protection, level landings at top/bottom
- **Code/Standards**: ADA/ABA Section 405, ANSI A117.1, IBC 1012
- **Related Details**: Stair & Ramp Railing Details
- **Drawing Complexity**: moderate

### Sub-group: Stair -- Handrail

#### STAIR - HANDRAIL WALL MOUNTED
- **File**: `STAIR - HANDRAIL WALL MOUNTED.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Round/oval handrail profile, wall bracket, concrete/CMU/stud wall, backing plate, screws/bolts
- **Key Elements**: Wall-mounted handrail bracket detail; shows handrail profile (1-1/4" to 2" graspable), 1-1/2" clearance from wall, bracket spacing, mounting height
- **Code/Standards**: IBC 1014 (handrails), ADA Section 505, 34"-38" height
- **Related Details**: Stair/Handrail Wall Mounted (duplicate naming), Stair Railing at Wall
- **Drawing Complexity**: simple

#### STAIR_HANDRAIL WALL MOUNTED
- **File**: `STAIR_HANDRAIL WALL MOUNTED.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Round handrail, wall bracket, wall assembly, backing plate
- **Key Elements**: Alternate version of wall-mounted handrail; may show different bracket type or wall condition
- **Code/Standards**: IBC 1014, ADA Section 505
- **Related Details**: Stair - Handrail Wall Mounted
- **Drawing Complexity**: simple

#### STAIR HANDRAIL TERMINATION
- **File**: `STAIR HANDRAIL TERMINATION.rvt`
- **Category**: Stair & Railing
- **Type**: section/elevation
- **Scale**: 3" = 1'-0"
- **Components Used**: Handrail profile, return-to-wall fitting, newel post, wall bracket
- **Key Elements**: Handrail end condition; shows 12" horizontal extension beyond top riser, return-to-wall or post-to-floor termination, transition from sloped to horizontal
- **Code/Standards**: IBC 1014.6 (extensions), ADA Section 505.10
- **Related Details**: Stair/Handrail Termination (duplicate)
- **Drawing Complexity**: simple

#### STAIR_HANDRAIL TERMINATION
- **File**: `STAIR_HANDRAIL TERMINATION.rvt`
- **Category**: Stair & Railing
- **Type**: section/elevation
- **Scale**: 3" = 1'-0"
- **Components Used**: Handrail profile, return fitting, wall/post
- **Key Elements**: Alternate handrail termination detail
- **Code/Standards**: IBC 1014.6, ADA Section 505.10
- **Related Details**: Stair Handrail Termination
- **Drawing Complexity**: simple

#### STAIR RAILING AT WALL
- **File**: `STAIR RAILING AT WALL.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Handrail, wall bracket, stud/CMU wall, backing plate, stair stringer
- **Key Elements**: Handrail mounting to wall at stair; shows bracket angle following stair slope, mounting height from nosing, clearance from wall surface
- **Code/Standards**: IBC 1014, ADA Section 505
- **Related Details**: Stair - Handrail Wall Mounted
- **Drawing Complexity**: simple

### Sub-group: Stair -- Railing (Freestanding)

#### STAIR - INNER RAILING
- **File**: `STAIR - INNER RAILING.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Steel post, top rail (handrail), intermediate rail/pickets, base plate, stair stringer, concrete landing
- **Key Elements**: Inner (open side) stair railing; shows post-to-stringer connection, handrail height from nosing line, guard infill spacing
- **Code/Standards**: IBC 1014/1015, 4" sphere rule, 34"-38" handrail height
- **Related Details**: Stair - Outer Railing, Typ. Handrail/Guardrail/Riser Details
- **Drawing Complexity**: moderate

#### STAIR - OUTER RAILING
- **File**: `STAIR - OUTER RAILING.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Steel post, top rail, guard rail, pickets, base plate, stair stringer, concrete slab edge
- **Key Elements**: Outer stair railing at open stairwell; shows guard height (42"), handrail height (34"-38"), post anchorage at stringer or slab edge
- **Code/Standards**: IBC 1014/1015
- **Related Details**: Stair - Inner Railing
- **Drawing Complexity**: moderate

#### STAIR & RAMP RAILING DETAILS
- **File**: `STAIR & RAMP RAILING DETAILS.rvt`
- **Category**: Stair & Railing
- **Type**: section/elevation
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Steel posts, handrails, guard rails, pickets, base plates, wall brackets, ramp slab
- **Key Elements**: Combined sheet showing stair and ramp railing configurations; multiple conditions including wall-mounted, freestanding, at ramp, at stair
- **Code/Standards**: IBC 1012/1014/1015, ADA Section 405/505
- **Related Details**: Section @ ADA Ramp, Stair - Inner Railing, Stair - Outer Railing
- **Drawing Complexity**: complex

#### TYP. HANDRAIL/GUARDRAIL/RISER DETAILS
- **File**: `TYP. HANDRAIL_GUARDRAIL_RISER DETAILS.rvt`
- **Category**: Stair & Railing
- **Type**: section/elevation
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Handrail profiles, guardrail assemblies, stair risers, nosing profiles, steel posts, pickets
- **Key Elements**: Comprehensive typical details for handrail profiles, guardrail assemblies, and riser/nosing conditions; likely multi-view sheet with plan, section, and elevation views. Preview shows guardrail at wall with post embedment in concrete, picket infill, and dual-rail configuration
- **Code/Standards**: IBC 1014/1015, ADA Section 505, ANSI A117.1
- **Related Details**: All stair and railing details
- **Drawing Complexity**: complex

### Sub-group: Stair -- Tread, Riser, Stringer

#### STAIR TREAD @ PLATFORM
- **File**: `STAIR TREAD @ PLATFORM.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Concrete stair, tread nosing, anti-slip strip, landing slab, mortar bed, tile/finish
- **Key Elements**: Stair tread transition at landing/platform; shows nosing profile, finish material transition, structural connection between stair flight and landing
- **Code/Standards**: IBC 1011 (stairways), 11" min tread depth, 4"-7" riser height
- **Related Details**: Stair/Pan Stair Tread/Riser
- **Drawing Complexity**: simple

#### STAIR_PAN STAIR STRINGER
- **File**: `STAIR_PAN STAIR STRINGER.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Steel channel stringer, steel pan treads, concrete fill, rebar mesh, steel plate connections, bolts
- **Key Elements**: Steel pan stair stringer detail; shows channel stringer profile, pan tread welded to stringer, concrete fill in pans, connection to landing beam
- **Code/Standards**: IBC 1011, AISC Steel Construction Manual
- **Related Details**: Stair/Pan Stair Tread/Riser, Stair/Pan Stair Termination
- **Drawing Complexity**: moderate

#### STAIR_PAN STAIR TERMINATION
- **File**: `STAIR_PAN STAIR TERMINATION.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Steel stringer, landing beam/angle, bolted connection, concrete slab, embed plate
- **Key Elements**: Connection of steel pan stair stringer to landing or floor slab; shows bearing detail, anchor bolt pattern, embed plate in concrete
- **Code/Standards**: IBC 1011, AISC
- **Related Details**: Stair/Pan Stair Stringer
- **Drawing Complexity**: moderate

#### STAIR_PAN STAIR TREAD/RISER
- **File**: `STAIR_PAN STAIR TREAD_RISER.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Steel pan, concrete fill, rebar mesh, nosing angle, riser plate
- **Key Elements**: Individual pan stair tread and riser; shows pan depth, concrete fill, nosing overhang, riser-to-tread weld connection
- **Code/Standards**: IBC 1011, uniform riser height requirement
- **Related Details**: Stair/Pan Stair Stringer
- **Drawing Complexity**: simple

### Sub-group: Stair -- Landing

#### STAIR - BASE LANDING
- **File**: `STAIR- BASE LANDING.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1/2" = 1'-0"
- **Components Used**: Concrete landing slab, steel stringer, foundation/slab-on-grade, dowels, nosing, rebar
- **Key Elements**: Bottom landing of stairway; shows stringer bearing on foundation, landing slab thickness, first riser, connection to floor slab
- **Code/Standards**: IBC 1011.6 (landings), min landing depth = stair width
- **Related Details**: Stair - Intermediate Landing Detail, Stair - Landing at Top
- **Drawing Complexity**: moderate

#### STAIR - INTERMEDIATE LANDING DETAIL
- **File**: `STAIR- INTERMEDIATE LANDING DETAIL.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1/2" = 1'-0"
- **Components Used**: Concrete landing slab, steel stringers (upper and lower flights), steel beams, hanger connections, rebar
- **Key Elements**: Mid-flight landing between stair runs; shows landing slab supported by steel beams, stringer connections at upper and lower flights, structural framing
- **Code/Standards**: IBC 1011.6
- **Related Details**: Stair - Base Landing, Stair - Landing at Top
- **Drawing Complexity**: moderate

#### STAIR - LANDING AT TOP
- **File**: `STAIR- LANDING AT TOP.rvt`
- **Category**: Stair & Railing
- **Type**: section
- **Scale**: 1/2" = 1'-0"
- **Components Used**: Concrete floor slab, steel stringer, landing angle/embed, nosing, rebar, connection hardware
- **Key Elements**: Top landing where stair meets floor level; shows stringer connection to floor slab edge, last riser, nosing at landing, structural embed
- **Code/Standards**: IBC 1011.6
- **Related Details**: Stair - Base Landing, Stair - Intermediate Landing Detail
- **Drawing Complexity**: moderate

---

## 3. FIRE PROTECTION DETAILS (10 files)

### Sub-group: Fire Stopping -- General

#### FIRE STOPPING DETAILS
- **File**: `FIRE STOPPING DETAILS.rvt`
- **Category**: Fire Protection
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Fire-rated wall/floor assemblies, fire caulk/sealant, mineral wool, intumescent strips, pipe/conduit sleeves
- **Key Elements**: Multiple firestop conditions on one sheet; shows typical head-of-wall, through-penetration, and joint conditions with UL-listed firestop systems
- **Code/Standards**: IBC Section 714, ASTM E814, UL firestop directory
- **Related Details**: Fire Stopping - Penetrations, Fire Stopping - Wall to Ceiling, Fire Stopping - Wall to Deck
- **Drawing Complexity**: complex

#### FIRE STOPPING - PENETRATIONS
- **File**: `FIRE STOPPING - PENETRATIONS.rvt`
- **Category**: Fire Protection
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Fire-rated wall/floor, pipe/conduit/duct penetration, firestop caulk, mineral wool packing, intumescent collar, steel sleeve
- **Key Elements**: Through-penetration firestop assemblies; shows pipe through wall, pipe through floor, conduit bundles, annular space fill requirements
- **Code/Standards**: IBC 714.4, ASTM E814 (F/T ratings), UL W-series (walls), UL C-series (floors)
- **Related Details**: Fire Stopping Details, Fire Stopping FW Detail - 1054
- **Drawing Complexity**: moderate

#### FIRE STOPPING - WALL TO CEILING
- **File**: `FIRE STOPPING - WALL TO CEILING.rvt`
- **Category**: Fire Protection
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Fire-rated stud wall, ceiling assembly, fire caulk/sealant, mineral wool, deflection track
- **Key Elements**: Head-of-wall firestop at ceiling intersection; shows deflection joint accommodating movement, fire sealant at gap, continuity of fire barrier above ceiling
- **Code/Standards**: IBC 714.5 (fire-resistant joint systems), ASTM E1966
- **Related Details**: Fire Stopping - Wall to Deck, Fire Stopping Details
- **Drawing Complexity**: moderate

#### FIRE STOPPING - WALL TO DECK
- **File**: `FIRE STOPPING - WALL TO DECK.rvt`
- **Category**: Fire Protection
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Fire-rated stud wall, concrete deck, fire sealant, mineral wool, deflection track, spray fireproofing
- **Key Elements**: Head-of-wall firestop at structural deck; shows joint between top of fire-rated wall and underside of concrete deck, sealant/mineral wool infill
- **Code/Standards**: IBC 714.5, ASTM E1966
- **Related Details**: Fire Stopping - Wall to Ceiling
- **Drawing Complexity**: moderate

### Sub-group: Fire Stopping -- UL Assemblies

#### FIRE STOPPING FW DETAIL - 1054
- **File**: `Fire Stopping FW Detail - 1054.rvt`
- **Category**: Fire Protection
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Fire-rated wall assembly, firestop system per UL Design 1054, fire caulk, mineral wool
- **Key Elements**: Specific UL-listed firestop system for floor/wall joint; references UL system number for code compliance documentation
- **Code/Standards**: UL Design No. 1054, IBC 714
- **Related Details**: Fire Stopping HW Detail - 1049
- **Drawing Complexity**: simple

#### FIRE STOPPING HW DETAIL - 1049
- **File**: `Fire Stopping HW Detail - 1049.rvt`
- **Category**: Fire Protection
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Fire-rated wall assembly, firestop system per UL Design 1049, fire caulk, mineral wool
- **Key Elements**: UL-listed head-of-wall firestop system; specific to HW (head-of-wall) joint condition
- **Code/Standards**: UL Design No. 1049, IBC 714
- **Related Details**: Fire Stopping FW Detail - 1054
- **Drawing Complexity**: simple

### Sub-group: Fire-Rated Assemblies

#### TYP. EPICORE SLAB UL DESIGN NO. D938
- **File**: `TYP. EPICORE SLAB UL DESIGN NO. D938.rvt`
- **Category**: Fire Protection
- **Type**: section
- **Scale**: 1" = 1'-0"
- **Components Used**: Epicore MSR composite floor deck, concrete topping, steel beams, spray fireproofing, rebar/mesh
- **Key Elements**: UL-listed fire-rated composite floor assembly; shows deck profile, concrete thickness, spray fireproofing on steel, restrained/unrestrained ratings
- **Code/Standards**: UL Design No. D938, IBC Table 722.2, ASTM E119
- **Related Details**: Typ. Steel Column and Beam Fireproofing
- **Drawing Complexity**: moderate

#### TYP. STEEL COLUMN AND BEAM FIREPROOFING
- **File**: `TYP. STEEL COLUMN AND BEAM FIREPROOFING.rvt`
- **Category**: Fire Protection
- **Type**: section
- **Scale**: 1" = 1'-0"
- **Components Used**: Steel wide-flange column, steel beam, spray-applied fire-resistive material (SFRM), thickness markers
- **Key Elements**: Fireproofing application on steel structural members; shows required SFRM thickness for rated assembly, coverage on all exposed surfaces, column vs. beam differences
- **Code/Standards**: IBC 722, UL X-series (columns), ASTM E119, AWCI 12-B
- **Related Details**: Typ. Epicore Slab UL Design No. D938
- **Drawing Complexity**: simple

#### DETAIL OF 2 HR FIRE RATED DUCT/WALL CONNECTION - UL U529
- **File**: `DETAIL OF 2 HR FIRE RATED DUCT _ WALL CONNECTION - UL U529.rvt`
- **Category**: Fire Protection
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Fire-rated wall, HVAC duct, fire damper, fire caulk, sheet metal collar, angle framing
- **Key Elements**: Duct penetration through 2-hour fire-rated wall; shows fire damper installation, duct connection to wall framing, firestop at perimeter, access panel location
- **Code/Standards**: UL U529, IBC 717 (fire dampers), NFPA 90A, SMACNA
- **Related Details**: Fire Stopping - Penetrations
- **Drawing Complexity**: complex

#### SKLAR UL DETAIL
- **File**: `SKLAR UL DETAIL.rvt`
- **Category**: Fire Protection
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Project-specific fire-rated assembly (Sklar brand), gypsum board layers, steel studs, insulation, UL-listed components
- **Key Elements**: Project-specific UL assembly detail; likely a proprietary partition or floor/ceiling assembly with specific layering requirements
- **Code/Standards**: UL fire resistance directory, IBC 722
- **Related Details**: Fire Stopping Details
- **Drawing Complexity**: moderate

---

## 4. MEP DETAILS (5 files)

### Sub-group: Plumbing

#### BACKFLOW PREVENTER DETAIL
- **File**: `BACKFLOW PREVENTER DETAIL.rvt`
- **Category**: MEP
- **Type**: section
- **Scale**: 1/2" = 1'-0"
- **Components Used**: Backflow preventer valve, piping, gate valves, test cocks, concrete pad, bollards, enclosure
- **Key Elements**: Backflow prevention device installation; shows valve orientation, test port locations, isolation valves, support/mounting, clearances for maintenance access
- **Code/Standards**: IPC Section 608, ASSE 1013/1015, local water authority requirements
- **Related Details**: Backflow Preventer Elevation, Backflow Preventer Plan
- **Drawing Complexity**: moderate

#### BACKFLOW PREVENTER ELEVATION
- **File**: `BACKFLOW PREVENTER ELEVATION.rvt`
- **Category**: MEP
- **Type**: elevation
- **Scale**: 1/2" = 1'-0"
- **Components Used**: Backflow preventer, piping, support frame, concrete pad, bollards
- **Key Elements**: Front elevation view of backflow preventer assembly; shows height from grade, pipe routing, valve accessibility
- **Code/Standards**: IPC Section 608, ASSE standards
- **Related Details**: Backflow Preventer Detail, Backflow Preventer Plan
- **Drawing Complexity**: simple

#### BACKFLOW PREVENTER PLAN
- **File**: `BACKFLOW PREVENTER PLAN.rvt`
- **Category**: MEP
- **Type**: plan
- **Scale**: 1/2" = 1'-0"
- **Components Used**: Backflow preventer, piping, concrete pad, bollards, enclosure footprint
- **Key Elements**: Plan view of backflow preventer installation; shows pipe routing, clearance dimensions, bollard locations, access requirements
- **Code/Standards**: IPC Section 608, local utility standards
- **Related Details**: Backflow Preventer Detail, Backflow Preventer Elevation
- **Drawing Complexity**: simple

### Sub-group: Mechanical

#### MECHANICAL DUCT ENCLOSURE DETAIL
- **File**: `MECHANICAL DUCT ENCLOSURE DETAIL.rvt`
- **Category**: MEP
- **Type**: section
- **Scale**: 1" = 1'-0"
- **Components Used**: HVAC duct, gypsum board enclosure, steel stud framing, fire caulk, access panels
- **Key Elements**: Fire-rated shaft/enclosure for mechanical ducts; shows stud framing around duct, gypsum board layers, fire caulk at penetrations, access panel locations
- **Code/Standards**: IBC 713 (shaft enclosures), NFPA 90A, SMACNA
- **Related Details**: Detail of 2 Hr Fire Rated Duct/Wall Connection
- **Drawing Complexity**: moderate

#### TYPICAL STANDPIPE
- **File**: `TYPICAL STANDPIPE.rvt`
- **Category**: MEP
- **Type**: diagram/section
- **Scale**: NTS (diagram) / 1/2" = 1'-0" (section)
- **Components Used**: Standpipe riser, hose valve connections, fire department connection (FDC), check valves, piping supports, floor penetrations
- **Key Elements**: Standpipe system riser diagram or section; shows riser through multiple floors, hose valve locations at each floor, FDC connection at base, pipe sizes, valve types. Preview shows multi-view sheet with riser diagram, connection details, and pipe hanger details
- **Code/Standards**: NFPA 14 (standpipe systems), IBC 905, IFC
- **Related Details**: Fire Protection details
- **Drawing Complexity**: complex

---

## 5. TYPICAL DETAILS (16 files)

### Sub-group: Expansion Joints

#### EXPANSION JOINT PLAN DTL 1
- **File**: `EXPANSION JOINT PLAN DTL 1.rvt`
- **Category**: Typical
- **Type**: plan
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Concrete slab, expansion joint cover, compressible filler, sealant, rebar discontinuity
- **Key Elements**: Plan view of expansion joint routing; shows joint width, cover plate alignment, corner conditions, transitions
- **Code/Standards**: ACI 318, IBC Chapter 19
- **Related Details**: Expansion Joint Plan DTL 2, Expansion Joint DTL
- **Drawing Complexity**: simple

#### EXPANSION JOINT PLAN DTL 2
- **File**: `EXPANSION JOINT PLAN DTL 2.rvt`
- **Category**: Typical
- **Type**: plan
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Concrete slab, expansion joint assembly, filler, sealant
- **Key Elements**: Alternate plan configuration for expansion joint; possibly showing different corner condition, tee intersection, or transition
- **Code/Standards**: ACI 318, IBC Chapter 19
- **Related Details**: Expansion Joint Plan DTL 1
- **Drawing Complexity**: simple

#### EXPANSION JOINT AT PLANTER
- **File**: `EXPANSION JOINT AT PLANTER.rvt`
- **Category**: Typical
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Concrete slab, planter curb, expansion joint, waterproofing, compressible filler, sealant
- **Key Elements**: Expansion joint where it intersects a planter; shows joint continuity through planter wall, waterproofing tie-in
- **Code/Standards**: ACI 318, IBC Chapter 15/19
- **Related Details**: Expansion Joint DTL
- **Drawing Complexity**: moderate

#### EXPANSION JOINT DTL
- **File**: `EXPANSION JOINT DTL.rvt`
- **Category**: Typical
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Concrete slab, expansion joint cover assembly, compressible filler, sealant, dowels
- **Key Elements**: Typical section through expansion joint; shows joint width, filler depth, cover plate type, sealant bead profile
- **Code/Standards**: ACI 318
- **Related Details**: Expansion Joint Plan DTLs, Expansion Joint Terminations
- **Drawing Complexity**: simple

#### EXPANSION JOINT TERMINATION
- **File**: `EXPANSION JOINT TERMINATION.rvt`
- **Category**: Typical
- **Type**: section/plan
- **Scale**: 3" = 1'-0"
- **Components Used**: Concrete slab, expansion joint, termination plate, sealant, compressible filler
- **Key Elements**: End condition of expansion joint at wall or edge; shows how joint terminates, cover plate end detail, sealant termination
- **Code/Standards**: ACI 318
- **Related Details**: Expansion Joint Termination 2
- **Drawing Complexity**: simple

#### EXPANSION JOINT TERMINATION 2
- **File**: `EXPANSION JOINT TERMINATION 2.rvt`
- **Category**: Typical
- **Type**: section/plan
- **Scale**: 3" = 1'-0"
- **Components Used**: Concrete slab, expansion joint, alternate termination plate, sealant
- **Key Elements**: Alternate expansion joint termination; different edge or wall condition
- **Code/Standards**: ACI 318
- **Related Details**: Expansion Joint Termination
- **Drawing Complexity**: simple

### Sub-group: Framing & Construction

#### TYPICAL FRAMING DETAILS
- **File**: `TYPICAL FRAMING DETAILS.rvt`
- **Category**: Typical
- **Type**: section
- **Scale**: 1" = 1'-0"
- **Components Used**: Metal studs, track, headers, blocking, gypsum board, screws, clip angles. Preview shows header detail with cripple studs, track-to-stud connection, and blocking requirements
- **Key Elements**: Standard metal stud framing conditions; shows typical header detail with king and cripple studs, track connections, stud-to-track fastening, blocking for fixtures
- **Code/Standards**: IBC Chapter 22 (steel), AISI S220 (cold-formed steel framing)
- **Related Details**: Typical Header Detail (preview), Typical Metal Stud Blocking (preview)
- **Drawing Complexity**: moderate

#### TYPICAL COVE DETAIL
- **File**: `TYPICAL COVE DETAIL.rvt`
- **Category**: Typical
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Wall base, cove base, flooring material, adhesive, concrete slab
- **Key Elements**: Cove base installation at wall-to-floor junction; shows base profile, adhesive application, flooring termination
- **Code/Standards**: Industry standard practice
- **Related Details**: Carpet/Tile Transition
- **Drawing Complexity**: simple

#### TYPICAL SHELF HEIGHTS @ UNITS
- **File**: `TYPICAL SHELF HEIGHTS @ UNITS.rvt`
- **Category**: Typical
- **Type**: elevation/diagram
- **Scale**: 1/4" = 1'-0"
- **Components Used**: Shelving, brackets, wall studs, blocking, closet rod, door/opening
- **Key Elements**: Standard shelf and closet rod heights for residential units; shows ADA-accessible and standard heights, dimensions from finished floor
- **Code/Standards**: ADA Section 811 (storage), ANSI A117.1, Fair Housing Act
- **Related Details**: Mounting Heights, FHA Unit Details
- **Drawing Complexity**: simple

### Sub-group: Flooring Transitions

#### CARPET/TILE TRANSITION
- **File**: `CARPET_TILE TRANSITION.rvt`
- **Category**: Typical
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Carpet, tile, transition strip, mortar bed, concrete slab, tack strip
- **Key Elements**: Transition between carpet and tile flooring; shows height differential management, transition strip profile, substrate preparation
- **Code/Standards**: ADA (1/4" max vertical change), IBC 1003.4
- **Related Details**: Tile/Carpet Transition
- **Drawing Complexity**: simple

#### TILE/CARPET TRANSITION
- **File**: `TILE_CARPET TRANSITION.rvt`
- **Category**: Typical
- **Type**: section
- **Scale**: 3" = 1'-0"
- **Components Used**: Tile, carpet, transition strip, mortar bed, concrete slab, pad
- **Key Elements**: Reverse direction tile-to-carpet transition; alternate profile or substrate condition
- **Code/Standards**: ADA, IBC 1003.4
- **Related Details**: Carpet/Tile Transition
- **Drawing Complexity**: simple

### Sub-group: ADA & Code Compliance

#### ADA PARKING STALL DETAIL
- **File**: `ADA PARKING STALL DETAIL.rvt`
- **Category**: Typical
- **Type**: plan
- **Scale**: 1/4" = 1'-0"
- **Components Used**: Parking striping, signage, access aisle, curb ramp, concrete/asphalt
- **Key Elements**: ADA-compliant parking stall layout; shows 8' min stall width (van: 11'), 5' access aisle (van: 8'), signage placement, surface slope requirements
- **Code/Standards**: ADA Section 502, ANSI A117.1, IBC 1106
- **Related Details**: ANSI Public Details
- **Drawing Complexity**: simple

#### ANSI PUBLIC DETAILS
- **File**: `ANSI PUBLIC DETAILS.rvt`
- **Category**: Typical
- **Type**: plan/diagram
- **Scale**: various
- **Components Used**: Diagrams showing clearances, turning radii, reach ranges, fixture layouts
- **Key Elements**: ANSI A117.1 accessibility reference details; shows wheelchair turning space, clear floor space, forward/side reach ranges, grab bar locations
- **Code/Standards**: ANSI A117.1, ADA/ABA, Fair Housing Act
- **Related Details**: ADA Parking Stall Detail, FHA Unit Details
- **Drawing Complexity**: moderate

#### FHA UNIT DETAILS
- **File**: `FHA UNIT DETAILS.rvt`
- **Category**: Typical
- **Type**: plan/diagram
- **Scale**: 1/4" = 1'-0"
- **Components Used**: Door clearances, kitchen layouts, bathroom layouts, turning spaces, floor space diagrams
- **Key Elements**: Fair Housing Act accessibility requirements for residential units; shows required clearances at doors, kitchens, bathrooms, accessible routes within units
- **Code/Standards**: Fair Housing Act, ANSI A117.1, HUD guidelines
- **Related Details**: ANSI Public Details, Typical Shelf Heights @ Units
- **Drawing Complexity**: moderate

### Sub-group: Standards & Reference

#### DRAFTING STANDARDS
- **File**: `DRAFTING STANDARDS.rvt`
- **Category**: Typical
- **Type**: diagram
- **Scale**: NTS
- **Components Used**: Line weights, text styles, dimension standards, symbol library, hatch patterns
- **Key Elements**: Office drafting standards reference sheet; shows line weight conventions, text heights, dimension styles, symbol legends, material hatch patterns
- **Code/Standards**: Office/firm standard
- **Related Details**: N/A
- **Drawing Complexity**: simple

#### GS+P BIM USE TERMS
- **File**: `GS+P BIM Use Terms.rvt`
- **Category**: Typical
- **Type**: diagram/text
- **Scale**: NTS
- **Components Used**: Text notes, diagrams
- **Key Elements**: BIM usage terms and conditions document (Glavovic Smith + Partners); shows legal/contractual language for BIM model usage, liability limitations
- **Code/Standards**: AIA E203 (BIM exhibit), AIA G202 (BIM protocol)
- **Related Details**: Drafting Standards
- **Drawing Complexity**: simple

---

## 6. STRUCTURAL DETAILS (1 file)

#### COLUMN ATTACHMENT DETAIL
- **File**: `COLUMN ATTACHMENT DETAIL.rvt`
- **Category**: Structural
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Steel column, base plate, anchor bolts, concrete pedestal/footing, grout pad, stiffener plates, gusset plates
- **Key Elements**: Steel column base plate connection to concrete foundation; shows base plate size, anchor bolt pattern, grout space, stiffener/gusset configuration, embed depth
- **Code/Standards**: AISC Steel Construction Manual, ACI 318 (anchorage), IBC Chapter 22
- **Related Details**: Steel Header to Concrete (99 - General)
- **Drawing Complexity**: moderate

---

## 7. SITE DETAILS (15 files)

### Sub-group: Fences & Screens

#### GREEN SCREEN DETAIL - FREESTANDING FENCE/SCREEN
- **File**: `GREEN SCREEN DETAIL- FREESTANDING FENCE_SCREEN.rvt`
- **Category**: Site
- **Type**: section/elevation
- **Scale**: 1/2" = 1'-0"
- **Components Used**: Steel posts, steel cable/mesh trellis, concrete footing, landscape planting, base plate
- **Key Elements**: Freestanding green screen/living wall structure; shows post embedment in footing, cable/mesh spacing for vine support, height, plant species notation
- **Code/Standards**: Local zoning (fence height), wind loading per ASCE 7
- **Related Details**: Typ Property Fence Detail, Wood Fence Detail
- **Drawing Complexity**: moderate

#### TYP PROPERTY FENCE DETAIL
- **File**: `TYP PROPERTY FENCE DETAIL.rvt`
- **Category**: Site
- **Type**: section/elevation
- **Scale**: 1/2" = 1'-0"
- **Components Used**: Fence posts (wood/metal), rails, pickets/panels, concrete footing, post cap
- **Key Elements**: Standard property line fence; shows post spacing, footing depth, rail connections, overall height, material specifications
- **Code/Standards**: Local zoning (setbacks, height limits), Florida Building Code (wind)
- **Related Details**: Wood Fence Detail, Double Gate Detail
- **Drawing Complexity**: simple

#### WOOD FENCE DETAIL
- **File**: `WOOD FENCE DETAIL.rvt`
- **Category**: Site
- **Type**: section/elevation
- **Scale**: 1/2" = 1'-0"
- **Components Used**: Pressure-treated wood posts, horizontal rails, vertical pickets, concrete footing, post cap, galvanized fasteners
- **Key Elements**: Wood privacy/picket fence construction; shows post embedment, rail-to-post connection, picket spacing, overall dimensions
- **Code/Standards**: Local zoning, AWPA (wood preservative), Florida Building Code (wind)
- **Related Details**: Typ Property Fence Detail
- **Drawing Complexity**: simple

#### DOUBLE GATE DETAIL
- **File**: `DOUBLE GATE DETAIL.rvt`
- **Category**: Site
- **Type**: elevation/plan
- **Scale**: 1/2" = 1'-0"
- **Components Used**: Gate frame (steel/aluminum), hinges, latch hardware, gate posts, drop rod, concrete footing
- **Key Elements**: Double-swing gate assembly; shows hinge placement, latch/lock hardware, clearance at bottom, post reinforcement, opening width
- **Code/Standards**: Local zoning, ADA (if at accessible route), NFPA 101 (egress gates)
- **Related Details**: Typ Property Fence Detail
- **Drawing Complexity**: moderate

### Sub-group: Dumpster Enclosure

#### DUMPSTER PLAN
- **File**: `DUMPSTER PLAN.rvt`
- **Category**: Site
- **Type**: plan
- **Scale**: 1/4" = 1'-0"
- **Components Used**: CMU/concrete walls, gate opening, concrete pad, bollards, drainage, striping
- **Key Elements**: Plan view of dumpster enclosure; shows wall layout, gate opening width, pad dimensions, truck access clearance, bollard locations
- **Code/Standards**: Local waste management requirements, ADA (accessible route around enclosure), fire department access
- **Related Details**: Dumpster Front Elevation, Dumpster Side Elevation, Dumpster Wall Section
- **Drawing Complexity**: simple

#### DUMPSTER FRONT ELEVATION
- **File**: `DUMPSTER FRONT ELEVATION.rvt`
- **Category**: Site
- **Type**: elevation
- **Scale**: 1/4" = 1'-0"
- **Components Used**: CMU/concrete walls, steel gates, gate hardware, wall cap, bollards
- **Key Elements**: Front elevation showing gate configuration, wall height, gate height, hardware locations, material callouts
- **Code/Standards**: Local waste management, zoning screening requirements
- **Related Details**: Dumpster Plan, Dumpster Side Elevation, Dumpster Wall Section
- **Drawing Complexity**: simple

#### DUMPSTER SIDE ELEVATION (TYP)
- **File**: `DUMPSTER SIDE ELEVATION (TYP).rvt`
- **Category**: Site
- **Type**: elevation
- **Scale**: 1/4" = 1'-0"
- **Components Used**: CMU/concrete wall, wall cap/coping, footing (implied), grade line
- **Key Elements**: Side view of enclosure wall; shows wall height, cap/coping detail, grade relationship, material specification
- **Code/Standards**: Local zoning, structural per wind zone
- **Related Details**: Dumpster Front Elevation, Dumpster Wall Section
- **Drawing Complexity**: simple

#### DUMPSTER WALL SECTION
- **File**: `DUMPSTER WALL SECTION.rvt`
- **Category**: Site
- **Type**: section
- **Scale**: 1" = 1'-0"
- **Components Used**: CMU wall, reinforcing (vertical rebar, bond beam), concrete footing, wall cap, concrete pad, gravel base
- **Key Elements**: Wall section through dumpster enclosure; shows CMU coursing, rebar placement, bond beam, footing size and depth, pad thickness, cap detail
- **Code/Standards**: IBC Chapter 21 (masonry), ACI 530/TMS 402
- **Related Details**: Dumpster Plan, Dumpster Front Elevation
- **Drawing Complexity**: moderate

### Sub-group: Paving & Hardscape

#### PAVERS DETAIL
- **File**: `PAVERS DETAIL.rvt`
- **Category**: Site
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Concrete/brick pavers, sand setting bed, aggregate base, geotextile fabric, compacted subgrade, edge restraint
- **Key Elements**: Typical paver installation cross-section; shows layer thicknesses, compaction requirements, edge restraint type, joint sand
- **Code/Standards**: ICPI (Interlocking Concrete Pavement Institute), ASTM C936
- **Related Details**: Typ Paver Edge Detail @ Driveways, Typ Paver Edge Detail @ Walkways
- **Drawing Complexity**: simple

#### TYP PAVER EDGE DETAIL @ DRIVEWAYS & PATIO
- **File**: `TYP PAVER EDGE DETAIL @ DRIVEWAYS & PATIO.rvt`
- **Category**: Site
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Pavers, sand bed, aggregate base, concrete edge restraint/curb, spike/adhesive
- **Key Elements**: Edge restraint at driveway/patio pavers; shows concrete edge band, restraint anchorage, transition to adjacent surface (asphalt/concrete)
- **Code/Standards**: ICPI, local paving standards
- **Related Details**: Pavers Detail, Typ Paver Edge Detail @ Walkways
- **Drawing Complexity**: simple

#### TYP PAVER EDGE DETAIL @ WALKWAYS
- **File**: `TYP PAVER EDGE DETAIL @ WALKWAYS.rvt`
- **Category**: Site
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Pavers, sand bed, aggregate base, edge restraint (aluminum/plastic/concrete), landscape edging
- **Key Elements**: Paver edge at pedestrian walkway; shows lighter-duty edge restraint vs. driveway condition, transition to landscape/lawn
- **Code/Standards**: ICPI, ADA (walkway surface requirements)
- **Related Details**: Pavers Detail, Typ Paver Edge Detail @ Driveways
- **Drawing Complexity**: simple

### Sub-group: Site Amenities

#### DRINKING FOUNTAIN DETAILS
- **File**: `DRINKING FOUNTAIN DETAILS.rvt`
- **Category**: Site
- **Type**: elevation/section
- **Scale**: 1/2" = 1'-0"
- **Components Used**: Drinking fountain unit, water supply, waste drain, concrete pad, anchor bolts
- **Key Elements**: Exterior drinking fountain installation; shows hi-lo fountain (ADA), mounting heights, water supply routing, waste drain connection, pad dimensions
- **Code/Standards**: ADA Section 602 (drinking fountains), IPC
- **Related Details**: ADA Sign Detail (99 - General)
- **Drawing Complexity**: moderate

#### MAIL BOXES
- **File**: `MAIL BOXES.rvt`
- **Category**: Site
- **Type**: elevation/plan
- **Scale**: 1/4" = 1'-0"
- **Components Used**: Cluster mailbox unit (CBU), concrete pad, bollards/posts, weather protection canopy (if any)
- **Key Elements**: USPS cluster box unit installation; shows mounting height, pad dimensions, accessible approach, postal service requirements
- **Code/Standards**: USPS STD-4C, ADA Section 309 (operable parts), ANSI A117.1
- **Related Details**: N/A
- **Drawing Complexity**: simple

#### TYP BOLLARD DETAIL
- **File**: `TYP BOLLARD DETAIL.rvt`
- **Category**: Site
- **Type**: section/elevation
- **Scale**: 1" = 1'-0"
- **Components Used**: Steel pipe bollard, concrete footing, concrete fill, cap plate, paint/sleeve, grade
- **Key Elements**: Standard bollard installation; shows pipe diameter, footing depth, concrete fill, height above grade, cap detail, paint specification
- **Code/Standards**: Local site requirements, DOT standards (if in ROW)
- **Related Details**: Dumpster Plan (bollards), Backflow Preventer (bollards)
- **Drawing Complexity**: simple

#### TRASH CHUTE & VENT DETAILS
- **File**: `TRASH CHUTE & VENT DETAILS.rvt`
- **Category**: Site
- **Type**: section/diagram
- **Scale**: 1/2" = 1'-0"
- **Components Used**: Trash chute (steel), intake doors at each floor, vent pipe, fire sprinkler head, compactor, concrete pad, shaft enclosure
- **Key Elements**: Trash chute system from intake to compactor; shows chute diameter, intake door at each floor, vent pipe to roof, sprinkler head at top, fire-rated shaft enclosure, compactor at base
- **Code/Standards**: IBC 713 (shaft enclosures), NFPA 82 (trash chutes), local fire codes
- **Related Details**: Mechanical Duct Enclosure Detail
- **Drawing Complexity**: complex

---

## 8. GENERAL DETAILS (10 files)

### Sub-group: ADA & Accessibility

#### ADA SIGN DETAIL
- **File**: `ADA SIGN DETAIL.rvt`
- **Category**: General
- **Type**: elevation/diagram
- **Scale**: 1" = 1'-0"
- **Components Used**: ADA-compliant signage panel, raised text/braille, mounting hardware, wall
- **Key Elements**: ADA signage mounting detail; shows sign placement height (48"-60" AFF to baseline of characters), location adjacent to latch side of door, sign dimensions
- **Code/Standards**: ADA Section 703, ANSI A117.1, IBC 1112
- **Related Details**: Mounting Heights, Wheelchair Elevation
- **Drawing Complexity**: simple

#### MOUNTING HEIGHTS
- **File**: `MOUNTING HEIGHTS.rvt`
- **Category**: General
- **Type**: elevation/diagram
- **Scale**: 1/4" = 1'-0"
- **Components Used**: Wall, fixtures (switches, outlets, thermostat, fire alarm pull), dimension strings. Preview shows mounting heights for various devices on a wall elevation with dimension callouts
- **Key Elements**: Standard mounting heights for electrical devices, accessories, and fixtures; shows AFF dimensions for switches (48"), outlets (18"), thermostats (48"), fire alarm pulls (48"-54")
- **Code/Standards**: ADA Section 308 (reach ranges), NEC, ANSI A117.1
- **Related Details**: Typ. Mounting Heights
- **Drawing Complexity**: simple

#### TYP. MOUNTING HEIGHTS
- **File**: `TYP. MOUNTING HEIGHTS.rvt`
- **Category**: General
- **Type**: elevation/diagram
- **Scale**: 1/4" = 1'-0"
- **Components Used**: Wall, fixtures, dimension strings
- **Key Elements**: Alternate or expanded version of mounting heights; may include additional fixture types or room-specific heights
- **Code/Standards**: ADA Section 308, NEC, ANSI A117.1
- **Related Details**: Mounting Heights
- **Drawing Complexity**: simple

#### WHEELCHAIR ELEVATION
- **File**: `wheelchair-elevation.rvt`
- **Category**: General
- **Type**: elevation/diagram
- **Scale**: NTS
- **Components Used**: Wheelchair profile diagram, dimension references, reach range indicators
- **Key Elements**: Reference diagram showing wheelchair user dimensions; forward reach, side reach, knee clearance, toe clearance, eye height -- used for verifying clearance requirements
- **Code/Standards**: ADA/ABA, ANSI A117.1
- **Related Details**: ADA Sign Detail, Mounting Heights
- **Drawing Complexity**: simple

### Sub-group: Balcony Edge

#### BALCONY EDGE DETAIL
- **File**: `BALCONY EDGE DETAIL.rvt`
- **Category**: General
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Concrete slab edge, waterproofing membrane, drip edge flashing, stucco/plaster finish, railing post base plate
- **Key Elements**: Balcony slab edge termination; shows waterproofing turn-down, drip edge profile, exterior finish at soffit, railing base plate integration
- **Code/Standards**: IBC Chapter 14 (exterior walls), Chapter 15 (waterproofing)
- **Related Details**: Balcony Edge Detail W/Tile
- **Drawing Complexity**: moderate

#### BALCONY EDGE DETAIL W/ TILE
- **File**: `BALCONY EDGE DETAIL W_ TILE.rvt`
- **Category**: General
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Concrete slab edge, waterproofing membrane, mortar bed, tile, drip edge, edge trim, railing post
- **Key Elements**: Balcony edge with tile finish; shows tile-to-edge trim transition, waterproofing under mortar bed, drip edge at slab soffit, tile overhang or metal edge strip
- **Code/Standards**: IBC Chapters 14/15, TCNA (tile installation)
- **Related Details**: Balcony Edge Detail
- **Drawing Complexity**: moderate

### Sub-group: Miscellaneous Architectural

#### DETAIL @ DECORATIVE BRACKET
- **File**: `DETAIL @ DECORATIVE BRACKET.rvt`
- **Category**: General
- **Type**: section/elevation
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: Decorative bracket (GFRC/FRP/cast stone), steel support angle, anchor bolts, wall assembly, sealant
- **Key Elements**: Ornamental bracket attachment to building facade; shows concealed steel support, anchor pattern, sealant joints, material specification
- **Code/Standards**: IBC Chapter 14 (veneer/cladding), wind loading per ASCE 7
- **Related Details**: N/A
- **Drawing Complexity**: moderate

#### DETAIL @ ELEVATOR ROOF
- **File**: `DETAIL @ ELEVATOR ROOF.rvt`
- **Category**: General
- **Type**: section
- **Scale**: 1/2" = 1'-0"
- **Components Used**: Elevator machine room walls, roof slab, waterproofing, roofing, parapet, access hatch, structural framing
- **Key Elements**: Section through elevator overrun/machine room roof; shows roof assembly, waterproofing, parapet height, ventilation, equipment access, structural clearances above cab
- **Code/Standards**: ASME A17.1 (elevator code), IBC Chapter 30 (elevators), IBC Chapter 15 (roofing)
- **Related Details**: N/A
- **Drawing Complexity**: complex

#### WHEEL STOP DETAIL
- **File**: `WHEEL STOP DETAIL.rvt`
- **Category**: General
- **Type**: section/plan
- **Scale**: 1" = 1'-0"
- **Components Used**: Pre-cast concrete or rubber wheel stop, anchor pins, concrete parking surface
- **Key Elements**: Wheel stop installation; shows anchor pin locations, setback from curb/wall, height, length, material specification
- **Code/Standards**: Local parking standards, ADA (accessible stalls may not use wheel stops per some jurisdictions)
- **Related Details**: ADA Parking Stall Detail
- **Drawing Complexity**: simple

#### BLOCK-UP DETAIL
- **File**: `BLOCK-UP DETAIL.rvt`
- **Category**: General
- **Type**: section
- **Scale**: 1-1/2" = 1'-0"
- **Components Used**: CMU block, mortar, rebar, concrete slab, waterproofing, sealant
- **Key Elements**: CMU infill/block-up condition; shows block coursing to close an opening or build up from slab, grouted cells, rebar dowels into slab, top connection to structure above
- **Code/Standards**: IBC Chapter 21 (masonry), ACI 530/TMS 402
- **Related Details**: Column Attachment Detail (17 - Structural)
- **Drawing Complexity**: simple

---

## PREVIEW-ONLY DETAILS (No matching .rvt in removed_2026)

The following previews exist in the preview directories but correspond to .rvt files in the main library (not removed_2026). They are listed here as cross-reference for the component vocabulary:

### 04 - Floor Details (previews without removed .rvt match)
- `Accessible Toilet Room Floor Plans.png` -- ADA toilet room layouts, wheelchair clearances, fixture placement (ADA Section 604)
- `Clear Floor Space, Accessible Route & Wheel Turning Space.png` -- ADA diagrams: 30"x48" clear floor space, 60" turning circle, 36" accessible route (ADA Sections 304/402/403)
- `CERAMIC TILE AT SHOWER.png` -- Shower pan section: waterproofing membrane, mortar bed, tile, curb, linear drain, backer board on studs
- `EXT. STOREFRONT SILL DETAIL @ FLOOR.png` -- Storefront system sill at floor slab: aluminum frame, thermal break, sealant, flashing, weep holes, sub-sill flashing
- `INT. STOREFRONT SILL DETAIL @ FLOOR.png` -- Interior storefront sill: aluminum frame seated on slab with shim, sealant, carpet/tile transition
- `PENETRATION THROUGH SLAB.png` -- Pipe penetration through concrete slab: sleeve, fire caulk, escutcheon plate, waterproofing collar
- `SLAB INFILL DETAIL - GENERAL.png` -- Slab infill at demolished opening: new rebar doweled into existing, formwork, concrete pour, finish patch
- `SLAB INFILL DETAIL - SOG.png` (+ variants .0004-.0006) -- Slab-on-grade infill: compacted fill, vapor barrier, rebar mesh, concrete, finish match
- `SLAB INFILL DETAIL - ELEVATED.png` -- Elevated slab infill: shows plan and section with rebar dowels, edge formwork, shoring requirements
- `SLAB REPAIR DETAIL.png` -- Concrete spall repair: remove loose concrete, expose rebar, apply bonding agent, patch with repair mortar, finish flush

### 14 - MEP Details (previews without removed .rvt match)
- `ELECTRICAL CONDUIT DETAIL - ACAI.png` -- Conduit penetration through slab: shows conduit stub-up, concrete pour-stop, firestop at penetration
- `ELECTRICAL RISER DIAGRAM.png` -- Electrical service riser diagram: shows main switchboard, distribution panels per floor, feeder sizes, metering
- `METALLIC ELECTRICAL OUTLET BOXES RECESSED IN FIRE BARRIERS.png` -- UL-listed electrical box installation in fire-rated walls: steel box with fire putty pads, proper spacing between boxes on opposite sides
- `PLUMBING VENT FLASHING.png` -- Roof vent pipe flashing: lead/rubber boot, counterflashing, sealant, vent pipe projection above roof
- `TYPICAL PLUMBING DETAILS.png` -- Multi-view plumbing sheet: pipe hanger types, expansion/contraction provisions, valve details, drain/waste/vent connections

### 15 - Typical Details (previews without removed .rvt match)
- `General Notes (Florida).png` -- Florida-specific general notes sheet: FBC references, wind speed, exposure category, HVHZ provisions
- `TYPICAL HEADER DETAIL.png` -- Metal stud header: track-within-track header assembly, cripple studs, clip angle connection
- `TYPICAL INTERIOR FURRING.png` -- Interior furring wall: hat channel/Z-furring on concrete/CMU, gypsum board, insulation, waterproofing
- `TYPICAL METAL STUD BLOCKING.png` -- Two conditions: flat blocking for grab bars/accessories and box blocking for heavy fixtures, both with stud reinforcement
- `TYPICAL MOUNTING HEIGHTS.png` -- Switch/outlet/device mounting: shows AFF dimensions with leader lines to wall elevation
- `TYPICAL PIPE HANGER DETAILS.png` -- Multiple hanger types: clevis, trapeze, roller, spring, with sizing notes and load ratings

### 99 - General Details (extensive preview library)
- `3-TIER LOCKER.png` -- Locker elevation: 3-tier stacked lockers with dimensions, ventilation, shelf, hook
- `ADA MOUNTING HEIGHTS WC ACCESSORIES.png` -- Restroom accessory mounting: toilet paper holder, grab bars, soap dispenser, mirror heights per ADA
- `A_C UNIT CURB DETAIL.png` -- Rooftop AC unit curb: steel curb on roof deck, insulation, flashing, counterflashing, vibration isolation
- `BA-BB.png` -- Building section showing multi-story balcony/corridor condition with railing, slab edges, waterproofing
- `common detail components.png` -- Reference sheet of common Revit detail components: angles, channels, plates, bolts, weld symbols
- `DB.png` -- Distribution board/electrical panel enclosure detail: panel mounting, conduit entry, clearance requirements
- `DRINKING FOUNTAIN ANCHORAGE.png` -- Wall-mounted fountain: anchor bolt pattern, backing plate, supply/waste connections
- `EXT. SLIDER HEAD DETAIL.png` -- Exterior sliding door head: track housing, flashing, header framing, waterproofing integration
- `FALL PROTECTION RAIL DETAIL.png` -- Roof fall protection railing: OSHA-compliant guardrail at parapet, post-to-structure connection
- `FIRE STOPPING DETAIL C-AJ-0043.png` -- UL-listed firestop: shows UL logo, system number, section through joint with sealant/mineral wool
- `GABLE END DETAIL.png` -- Roof gable construction: rafter/truss framing at gable wall, sheathing, fascia, soffit, ventilation
- `Limits of Protruding Objects into Circulation Paths.png` -- ADA protruding objects: max 4" projection between 27"-80" AFF, cane detection
- `MARBLE THRESHOLD.png` -- Marble threshold at doorway: mortar bed, threshold profile (beveled), waterproofing beneath, sealant at jambs
- `OVER FLOW SCUPPER DETAIL.png` -- Overflow scupper at parapet: shows primary drain, secondary/emergency scupper through parapet, conductor, flashing
- `PENETRATION DETAIL C-AJ-1064.png` -- UL-listed penetration firestop: pipe through fire-rated wall, annular space fill, intumescent collar
- `PENETRATION DETAIL WL 1158.png` -- UL WL 1158 system: metallic pipe through gypsum wall, firestop sealant, mineral wool backing
- `PENETRATION FIRESTOP AND UL JOINT FIRESTOP SCHEDULE.png` -- Schedule/table: lists all UL system numbers used on project with conditions, materials, ratings
- `PRE-FORMED PIPE DETAIL.png` -- Pre-formed pipe penetration: shows factory-formed pipe boot through roof/wall, sealant, flashing collar
- `RECESSED LIGHT FIXTURE.png` -- Isometric: recessed can light in ceiling grid, IC-rated housing, thermal barrier, wiring
- `REINFORCED CONC. REPAIR.png` -- Concrete repair procedure: saw cut perimeter, remove deteriorated concrete, clean/coat rebar, apply repair mortar
- `RUBBER BASE.png` -- Rubber wall base installation: shows cove base at wall-floor junction, adhesive, corner conditions
- `SANITARY ISOMETRIC DIAGRAM.png` -- Plumbing waste isometric: fixture connections, vent stacks, cleanouts, pipe sizes
- `SD0201.png` -- Opening header details: multiple conditions for wall openings with steel lintels and wood headers
- `SD0204.png` -- Wall/partition sections: multiple partition types with material callouts, fire rating, STC rating
- `SD0301.png` -- Floor/ceiling assembly sections: concrete slab with various ceiling systems, fire-rated assemblies
- `SD0502.png` -- Roof parapet/edge details: multiple conditions showing flashing, coping, counterflashing, membrane termination
- `SD0508.png` -- Roof penetration/curb details: multiple equipment curb conditions, pipe penetrations, expansion joints
- `STEEL HEADER TO CONCRETE.png` -- Steel lintel/header bearing on concrete: base plate on CMU/concrete, bearing length, grout, anchor bolts
- `STUD REINFORCEMENT.png` -- Heavy-gauge stud reinforcement at openings and load points: nested studs, built-up jambs
- `SUSPENDED LIGHT FIXTURE.png` -- Pendant light: suspension cables from structure, junction box, ceiling penetration, seismic bracing
- `TYP. FASTENING DETAIL _ NOTES.png` -- Fastener schedule: screw types, anchor types, spacing requirements, pull-out values
- `TYP. GUTTER DETAIL.png` -- Metal gutter at eave: gutter profile, hanger spacing, downspout, flashing integration with roofing
- `UL DETAIL 505.png` -- UL fire-resistance assembly reference sheet: multiple UL system configurations in grid layout
- `WOOD TRUSS BRIDGING DETAIL.png` -- Wood truss lateral bracing: continuous bridging between trusses (text only, minimal graphics)

---

## CROSS-REFERENCE: COMPONENT LIBRARY USAGE

Based on preview analysis, these categories heavily use the following from the 87-family detail component library:

| Component Family | Used In Categories |
|---|---|
| Concrete/slab hatching | Floor, Fire Protection, Structural, Site |
| Steel shapes (angles, channels, plates) | Stair & Railing, Structural, General |
| Waterproofing membrane (line/hatch) | Floor, Stair & Railing, General |
| Metal studs/track | Typical, Fire Protection, MEP |
| Gypsum board layers | Fire Protection, Typical, MEP |
| Pipe/conduit profiles | MEP, Fire Protection, Floor |
| Masonry/CMU hatching | Site, General, Structural |
| Rebar/reinforcing | Floor, Structural, Site |
| Tile/mortar bed | Floor, General |
| Sealant/caulk (bead profile) | All categories |
| Fasteners (bolts, screws, anchors) | Structural, Stair & Railing, General |
| Insulation (batt/rigid) | Fire Protection, Typical, MEP |
| Flashing profiles | Floor, General, Site |
| Handrail/guardrail profiles | Stair & Railing |

---

## STATISTICS

| Category | Files | Has Previews | Avg Complexity |
|---|---|---|---|
| 04 - Floor Details | 14 | Yes (13 previews, mostly from main library) | moderate |
| 07 - Stair & Railing | 27 | Yes (1 preview) | moderate |
| 18 - Fire Protection | 10 | No | moderate |
| 14 - MEP Details | 5 | Yes (5 previews, from main library) | moderate |
| 15 - Typical Details | 16 | Yes (6 previews, from main library) | simple |
| 17 - Structural Details | 1 | No | moderate |
| 19 - Site Details | 15 | No | simple-moderate |
| 99 - General Details | 10 | Yes (34 previews, from main library) | simple-moderate |
| **TOTAL** | **98** | | |
