# Bathroom Details Catalog

**Source:** BD Architect Detail Library 2025
**Category:** 12 - Bathroom Details
**Total Files:** 37 .rvt details + 7 preview images
**Last Updated:** 2026-03-05

---

## RVT Detail Files (removed_2026/)

### 3D BATHROOM DETAIL
- **File**: 3D BATHROOM DETAIL.rvt
- **Type**: 3D (isometric/axonometric)
- **Fixture/Assembly**: complete bathroom layout
- **Waterproofing**: membrane at wet areas, shower pan
- **Components Used**: tub/shower, toilet, vanity, tile, cement board, framing
- **Code Requirements**: clearances, fixture spacing per IPC
- **Drawing Complexity**: complex

### AMENITIES RESTROOM VANITY SINK
- **File**: AMENITIES RESTROOM VANITY SINK.rvt
- **Type**: section
- **Fixture/Assembly**: vanity with undermount sink
- **Waterproofing**: backsplash sealant, countertop edge seal
- **Components Used**: vanity cabinet, solid surface countertop, undermount sink, supply/drain lines, mirror
- **Code Requirements**: ADA if accessible restroom, hot water max 120F
- **Drawing Complexity**: moderate

### BI-FOLD DOORS WITH TRANSOM TUBE
- **File**: BI-FOLD DOORS W_ TRANSOM TUBE.rvt
- **Type**: section
- **Fixture/Assembly**: shower enclosure bi-fold door with transom
- **Waterproofing**: gasket at door frame, weep to interior
- **Components Used**: bi-fold glass door, transom tube/bar, hinges, gaskets, frame channel
- **Code Requirements**: tempered/safety glass per IBC 2406
- **Drawing Complexity**: complex

### DOOR JAMB @ RESTROOMS
- **File**: DOOR JAMB @ RESTROOMS.rvt
- **Type**: section (jamb detail)
- **Fixture/Assembly**: restroom door frame condition
- **Waterproofing**: moisture-resistant GWB at wet side
- **Components Used**: hollow metal frame, MR drywall, tile wainscot, cement board substrate
- **Code Requirements**: ADA clearances at door, maneuvering space
- **Drawing Complexity**: moderate

### FOLDING SHOWER GLASS DOOR DETAIL
- **File**: FOLDING SHOWER GLASS DOOR DETAIL.rvt
- **Type**: section
- **Fixture/Assembly**: shower enclosure folding glass door
- **Waterproofing**: bottom sweep seal, jamb gasket
- **Components Used**: tempered glass panel, pivot hinges, sweep seal, header channel, wall channel
- **Code Requirements**: tempered glass, door swing out per code
- **Drawing Complexity**: moderate

### GRABBAR
- **File**: GRABBAR.rvt
- **Type**: section/elevation
- **Fixture/Assembly**: grab bar mounting detail
- **Waterproofing**: sealant at penetrations through tile/membrane
- **Components Used**: stainless steel grab bar, blocking (3/4" plywood), lag screws, tile, cement board
- **Code Requirements**: ADA - 1-1/4" to 1-1/2" dia, 1-1/2" clearance from wall, 250 lb load
- **Drawing Complexity**: simple

### KNEE WALL DETAIL
- **File**: KNEE WALL DETAIL.rvt
- **Type**: section
- **Fixture/Assembly**: shower knee wall / half wall
- **Waterproofing**: membrane continuous over knee wall cap, tile waterproof membrane
- **Components Used**: wood/metal stud framing, cement board, tile, waterproof membrane, cap tile
- **Code Requirements**: min height per design, cap slope for drainage
- **Drawing Complexity**: moderate

### LOCATION OF GRAB BARS (FOR ALL RESIDENTIAL UNITS)
- **File**: LOCATION OF GRAB BARS (FOR ALL RESIDENTIAL UNITS).rvt
- **Type**: elevation/plan
- **Fixture/Assembly**: grab bar layout diagram
- **Waterproofing**: not applicable (layout diagram)
- **Components Used**: grab bars (horizontal, vertical, angled), blocking zones
- **Code Requirements**: ADA/FHA - side wall 42" min, rear wall 36" min, 33-36" AFF mounting height
- **Drawing Complexity**: simple

### RESTROOM PARTITION DETAILS
- **File**: RESTROOM PARTITION DETAILS.rvt
- **Type**: section/plan
- **Fixture/Assembly**: toilet partition system
- **Waterproofing**: not applicable
- **Components Used**: HDPE/phenolic partitions, pilasters, headrail, brackets, anchors
- **Code Requirements**: ADA stall 60" wide x 59" deep min, 9" AFF toe clearance
- **Drawing Complexity**: moderate

### RESTROOM PARTITION ELEVATION DETAILS
- **File**: RESTROOM PARTITION ELEVATION DETAILS.rvt
- **Type**: elevation
- **Fixture/Assembly**: toilet partition elevation views
- **Waterproofing**: not applicable
- **Components Used**: partition panels, pilasters, door hardware, coat hook, indicator lock
- **Code Requirements**: partition height 58" typ, 12" AFF gap, ADA door pull/latch
- **Drawing Complexity**: moderate

### SECTION @ RESTROOM BASE CABINET W/ TRASH DROP & TOWEL DISPENSER
- **File**: SECTION @ RESTROOM BASE CABINET W_TRASH DROP & TOWEL DISPENSER1.rvt
- **Type**: section
- **Fixture/Assembly**: restroom vanity cabinet with integrated accessories
- **Waterproofing**: backsplash sealant, countertop edge seal
- **Components Used**: base cabinet, countertop, trash chute, paper towel dispenser recess, plumbing
- **Code Requirements**: ADA if accessible, trash opening height per accessibility
- **Drawing Complexity**: complex

### SECTION @ TYPICAL SINK VANITY IN AMENITIES BATHROOMS
- **File**: SECTION @ TYPICAL SINK VANITY IN AMENITIES BATHROOMS.rvt
- **Type**: section
- **Fixture/Assembly**: amenity bathroom vanity
- **Waterproofing**: backsplash seal, countertop waterproofing
- **Components Used**: vanity cabinet, stone/solid surface top, undermount sink, plumbing, mirror, sconce
- **Code Requirements**: fixture count per occupancy, ADA at accessible units
- **Drawing Complexity**: moderate

### SHOWER ADJACENT TO BATHTUB DETAIL
- **File**: SHOWER ADJACENT TO BATHTUB DETAIL.rvt
- **Type**: section
- **Fixture/Assembly**: shower-tub transition condition
- **Waterproofing**: continuous membrane from shower across tub deck, flashing at transition
- **Components Used**: shower pan, tub, cement board, tile, waterproof membrane, transition trim
- **Code Requirements**: continuous waterproofing, slope to drain
- **Drawing Complexity**: complex

### SHOWER CURB / GLAZING DETAIL
- **File**: SHOWER CURB_GLAZING DETAIL.rvt
- **Type**: section
- **Fixture/Assembly**: shower curb with glass panel
- **Waterproofing**: membrane over curb, dam at glass channel, slope to interior
- **Components Used**: concrete/wood curb, waterproof membrane, glass panel, U-channel, sealant, tile
- **Code Requirements**: curb height 2" min above finished floor, membrane extends min 3" up walls
- **Drawing Complexity**: moderate

### SHOWER DETAIL (TYP.)
- **File**: SHOWER DETAIL (TYP.).rvt
- **Type**: section
- **Fixture/Assembly**: typical shower wall/floor assembly
- **Waterproofing**: sheet/liquid membrane, pre-slope, shower pan liner
- **Components Used**: cement board, waterproof membrane, tile, thin-set, pre-slope mortar, drain
- **Code Requirements**: 1/4" per foot slope to drain, membrane test required
- **Drawing Complexity**: moderate

### SHOWER DETAIL
- **File**: SHOWER DETAIL.rvt
- **Type**: section
- **Fixture/Assembly**: shower wall-to-floor transition
- **Waterproofing**: membrane at wall/floor intersection, pan liner
- **Components Used**: cement board, tile, membrane, mortar bed, drain body, clamp ring
- **Code Requirements**: shower pan liner, slope to drain, water test
- **Drawing Complexity**: moderate

### SHOWER DTL
- **File**: SHOWER DTL.rvt
- **Type**: section
- **Fixture/Assembly**: shower detail (abbreviated)
- **Waterproofing**: membrane system, drain connection
- **Components Used**: cement board, tile, waterproof membrane, mortar, drain
- **Code Requirements**: slope, membrane, drain per IPC
- **Drawing Complexity**: moderate

### SHOWER GLASS DETAIL WITH PARTIAL WALL
- **File**: SHOWER GLASS DETAIL WITH PARTIAL WALL.rvt
- **Type**: section
- **Fixture/Assembly**: glass panel mounted on partial/knee wall
- **Waterproofing**: membrane on knee wall cap, sealant at glass channel
- **Components Used**: tempered glass panel, U-channel, knee wall framing, cement board, tile, sealant
- **Code Requirements**: tempered glass, stable mounting, water containment
- **Drawing Complexity**: moderate

### SHOWER GLASS DOOR DETAIL
- **File**: SHOWER GLASS DOOR DETAIL.rvt
- **Type**: section
- **Fixture/Assembly**: frameless/semi-frameless glass shower door
- **Waterproofing**: bottom sweep, jamb seals, sill dam
- **Components Used**: tempered glass door, pivot/hinge hardware, sweep seal, drip rail, wall clamp
- **Code Requirements**: tempered/safety glass, door swings outward
- **Drawing Complexity**: moderate

### SHOWER GRAB BAR
- **File**: SHOWER GRAB BAR.rvt
- **Type**: section/elevation
- **Fixture/Assembly**: grab bar in shower (wet area)
- **Waterproofing**: sealant around mounting flanges, membrane behind mounting plate
- **Components Used**: stainless grab bar, backing plate, through-bolt/lag, blocking, cement board, tile
- **Code Requirements**: ADA - 250 lb load test, 1-1/4" to 1-1/2" dia, height per ADA 604/608
- **Drawing Complexity**: simple

### SHOWER NICHE
- **File**: SHOWER NICHE.rvt
- **Type**: section
- **Fixture/Assembly**: recessed shower niche/shelf
- **Waterproofing**: membrane continuous into niche cavity, all 5 sides waterproofed, slope bottom shelf
- **Components Used**: framing box-out, cement board liner, waterproof membrane, tile, slope mortar
- **Code Requirements**: slope niche bottom 1/4" per foot toward shower, fully waterproofed
- **Drawing Complexity**: moderate

### SHOWER PAN DETAIL (TYPICAL)
- **File**: SHOWER PAN DETAIL (TYPICAL).rvt
- **Type**: section
- **Fixture/Assembly**: shower pan/receptor assembly
- **Waterproofing**: PVC/CPE pan liner, pre-slope, weep holes at drain, dam corners
- **Components Used**: pre-slope mortar bed, pan liner, clamp drain, top mortar bed, tile, weep holes
- **Code Requirements**: liner water test 24 hrs, 1/4" per foot slope, liner 3" min up walls
- **Drawing Complexity**: complex

### SHOWER STEAM DOOR
- **File**: SHOWER STEAM DOOR.rvt
- **Type**: section
- **Fixture/Assembly**: steam shower enclosure door
- **Waterproofing**: full perimeter gasket, threshold dam, vapor seal
- **Components Used**: tempered glass door, steam-rated gaskets, transom panel, threshold, frame
- **Code Requirements**: full enclosure seal for steam containment, tempered glass, ceiling vapor barrier
- **Drawing Complexity**: complex

### SHOWER CURB AT TYPICAL SHOWER DOOR
- **File**: SHOWER_CURB AT TYPICAL SHOWER DOOR.rvt
- **Type**: section
- **Fixture/Assembly**: curb at shower door threshold
- **Waterproofing**: membrane wraps over curb, dam at both sides
- **Components Used**: wood/concrete curb, waterproof membrane, tile, door track/channel, sealant
- **Code Requirements**: curb height, membrane continuity, ADA - curbless option for accessible
- **Drawing Complexity**: moderate

### SHOWER CURB AT SHOWER ENCLOSURE / BATHROOM OR TOILET ROOM
- **File**: SHOWER_CURB AT SHOWER ENCLOSURE _ BATHROOM OR TOILET ROOM.rvt
- **Type**: section
- **Fixture/Assembly**: shower curb at enclosure perimeter
- **Waterproofing**: membrane over curb to both sides, corner dam
- **Components Used**: curb framing, membrane, tile, transition strip, mortar bed
- **Code Requirements**: curb slope, membrane continuity, floor transition
- **Drawing Complexity**: moderate

### SHOWER ENCLOSURE TRANSITION AT TOILET DOOR
- **File**: SHOWER_ENCLOSURE TRANSITION AT TOILET DOOR.rvt
- **Type**: section
- **Fixture/Assembly**: transition where shower enclosure meets restroom door
- **Waterproofing**: membrane termination, threshold transition
- **Components Used**: shower enclosure frame, door frame, threshold, waterproof membrane, transition trim
- **Code Requirements**: water containment, threshold height
- **Drawing Complexity**: moderate

### GUESTROOM SHOWER TUB SECTION
- **File**: SHOWER_GUESTROOM SHOWER TUB SECTION.rvt
- **Type**: section
- **Fixture/Assembly**: hotel guestroom shower/tub combo
- **Waterproofing**: tub flange seal, cement board to tub lip, membrane above tub
- **Components Used**: alcove tub, shower valve, shower head, cement board, tile, curtain rod, GWB above
- **Code Requirements**: anti-scald valve, grab bar blocking, slip-resistant surface
- **Drawing Complexity**: moderate

### SHOWER HEAD DETAIL 1
- **File**: SHOWER_HEAD DETAIL1.rvt
- **Type**: section (enlarged)
- **Fixture/Assembly**: shower head rough-in and trim
- **Waterproofing**: sealant at pipe penetration through membrane
- **Components Used**: shower arm, escutcheon, blocking, supply pipe, cement board, tile
- **Code Requirements**: shower head height 80" AFF typ, hand shower 48" AFF for ADA
- **Drawing Complexity**: simple

### SHOWER HEAD DETAIL 2
- **File**: SHOWER_HEAD DETAIL2.rvt
- **Type**: section (enlarged)
- **Fixture/Assembly**: shower head rough-in variant
- **Waterproofing**: sealant at pipe penetration
- **Components Used**: shower arm, escutcheon, blocking, supply pipe, wall assembly
- **Code Requirements**: shower head height per design, ADA hand shower option
- **Drawing Complexity**: simple

### SHOWER VALVE DETAIL 1
- **File**: SHOWER_VALVE DETAIL1.rvt
- **Type**: section (enlarged)
- **Fixture/Assembly**: shower valve rough-in and trim
- **Waterproofing**: membrane sealed around valve body
- **Components Used**: pressure-balance valve, escutcheon, supply pipes, blocking, cement board, tile
- **Code Requirements**: anti-scald/pressure-balance valve required (IPC 424.3), 38-48" AFF mounting
- **Drawing Complexity**: simple

### SHOWER VALVE DETAIL 2
- **File**: SHOWER_VALVE DETAIL2.rvt
- **Type**: section (enlarged)
- **Fixture/Assembly**: shower valve rough-in variant
- **Waterproofing**: membrane around valve penetration
- **Components Used**: thermostatic valve, escutcheon, supply pipes, blocking
- **Code Requirements**: anti-scald valve, accessible reach range for ADA
- **Drawing Complexity**: simple

### STORE FRONT / DETAIL @ INTERMEDIATE TUBE
- **File**: STORE FRONT_DETAIL @ INTERM. TUBE.rvt
- **Type**: section
- **Fixture/Assembly**: shower storefront-style glass at intermediate mullion
- **Waterproofing**: gaskets, weep system, sealant at frame
- **Components Used**: aluminum tube/mullion, glass panel, gaskets, setting blocks
- **Code Requirements**: tempered glass, mullion structural capacity
- **Drawing Complexity**: moderate

### TOILET ACCESSORIES ELEVATION
- **File**: Toilet_Accessories_Elevation_4020.rvt
- **Type**: elevation
- **Fixture/Assembly**: toilet accessory mounting layout
- **Waterproofing**: not applicable
- **Components Used**: toilet paper holder, grab bars, coat hook, seat cover dispenser, sanitary napkin
- **Code Requirements**: ADA mounting heights (TP holder 19" min AFF, grab bar 33-36" AFF)
- **Drawing Complexity**: simple

### TUB DETAIL
- **File**: TUB DETAIL.rvt
- **Type**: section
- **Fixture/Assembly**: bathtub installation
- **Waterproofing**: tub flange seal to wall, moisture barrier behind cement board
- **Components Used**: alcove/freestanding tub, cement board, tile, mortar bed, drain, overflow
- **Code Requirements**: overflow required, access panel for plumbing, anti-scald valve
- **Drawing Complexity**: moderate

### TYP. ADA VANITY DETAIL
- **File**: TYP. ADA VANITY DETAIL.rvt
- **Type**: section
- **Fixture/Assembly**: ADA-compliant vanity
- **Waterproofing**: backsplash sealant
- **Components Used**: wall-mount bracket, countertop, undermount sink, insulated pipes, lever faucet
- **Code Requirements**: ADA - 34" max AFF, 27" knee clearance, 8" deep at knee, insulated pipes
- **Drawing Complexity**: moderate

### TYPICAL BATH TUB DECK DETAIL
- **File**: TYPICAL BATH TUB DECK DETAIL.rvt
- **Type**: section
- **Fixture/Assembly**: tub deck/surround
- **Waterproofing**: membrane under deck tile, slope to tub, dam at edges
- **Components Used**: framing, plywood deck, membrane, mortar bed, tile, tub, access panel
- **Code Requirements**: structural support for water load, access to plumbing
- **Drawing Complexity**: complex

### TYPICAL MASTER BATH TUB DECK DETAIL
- **File**: TYPICAL MASTER BATH TUB DECK DETAIL-1.rvt
- **Type**: section
- **Fixture/Assembly**: master bath tub deck (upgraded)
- **Waterproofing**: membrane, slope to tub, waterproof backer at splash zone
- **Components Used**: framing, plywood deck, membrane, stone/tile, drop-in tub, access panel, step
- **Code Requirements**: structural support, access panel, step height per code
- **Drawing Complexity**: complex

---

## Preview-Only Details

These details have preview PNGs but correspond to library details (may overlap with .rvt files above or exist in the main library).

### FOLDING SHOWER SEAT
- **File**: (preview only)
- **Type**: section
- **Fixture/Assembly**: ADA folding shower seat
- **Waterproofing**: sealant at wall bracket penetrations, membrane behind mounting
- **Components Used**: folding seat mechanism, wall bracket, blocking (3/4" plywood full bay), stainless hardware
- **Code Requirements**: ADA - 17-19" AFF seat height, 250 lb load capacity, L-shaped or rectangular
- **Drawing Complexity**: moderate

### INPRO ADA SHOWER PAN
- **File**: (preview only)
- **Type**: section
- **Fixture/Assembly**: prefabricated ADA shower receptor
- **Waterproofing**: integral pan with pre-formed slope, membrane flange at walls
- **Components Used**: Inpro ADA receptor, trench drain, tile flange, wall membrane connection
- **Code Requirements**: ADA - curbless/roll-in, 1/2" max threshold, 1/4" per foot slope
- **Drawing Complexity**: moderate

### TYPICAL SHOWER PAN (Multiple Variants)
- **File**: (preview only - 5 variants: Standard, 1, 1.0007, 1.0008, 1.0009)
- **Type**: section
- **Fixture/Assembly**: conventional shower pan assembly
- **Waterproofing**: PVC/CPE liner, pre-slope mortar, clamp drain, weep holes, liner up walls 3" min
- **Components Used**: pre-slope mortar bed, pan liner, clamp ring drain, top mortar bed, tile
- **Code Requirements**: 24-hr water test, 1/4" per foot slope, weep holes at drain, liner membrane
- **Drawing Complexity**: moderate

---

## Summary Statistics

| Fixture/Assembly Category | Count |
|--------------------------|-------|
| Shower (pan, curb, enclosure, assembly) | 16 |
| Shower hardware (valve, head, grab bar) | 6 |
| Shower door/glass | 5 |
| Bathtub | 4 |
| Vanity/sink | 4 |
| Grab bar/accessory | 3 |
| Partition | 2 |
| Door/frame | 2 |
| Layout/3D | 2 |
| **Total** | **44** |

| Code/ADA Details | Count |
|-----------------|-------|
| ADA-specific | 7 |
| Waterproofing-critical | 20 |
| Tempered glass required | 5 |

| Drawing Type | Count |
|-------------|-------|
| Section | 33 |
| Elevation | 3 |
| Plan/layout | 2 |
| 3D | 1 |
| Enlarged detail | 5 |
