# Cabinetry & Millwork Detail Catalog

**Source:** BD Architect Detail Library 2025
**Category:** 02 - Cabinetry & Millwork
**Total Files:** 15 .rvt details + 35 preview images
**Last Updated:** 2026-03-05

---

## RVT Detail Files (removed_2026/)

### BANQUETTE / BENCH SECTION
- **File**: BANQUETTE_ BENCH SECTION.rvt
- **Type**: section
- **Cabinet Type**: specialty (built-in seating)
- **Components Used**: wood framing, plywood seat/back, upholstery, blocking, finish trim
- **Key Elements**: seat height, back angle, support framing, wall attachment, cushion profile
- **Dimensions**: seat height ~18", seat depth ~18-20", back height varies
- **ADA**: not applicable (seating, not accessible cabinet)
- **Drawing Complexity**: moderate

### BAR SECTION
- **File**: BAR SECTION.rvt
- **Type**: section
- **Cabinet Type**: specialty (bar counter)
- **Components Used**: base cabinet, bar top, foot rail bracket, plywood substrate, finish materials
- **Key Elements**: bar top overhang, foot rail, drink rail, under-bar shelving, sink rough-in
- **Dimensions**: bar top height 42", drink rail, knee space
- **ADA**: ADA bar section may require 34" lowered portion with knee clearance
- **Drawing Complexity**: complex

### BUILT-IN LINEN / PANTRY @ UNITS (Copy 1)
- **File**: BUILT-IN LINEN _PANTRY @ UNITS Copy 1.rvt
- **Type**: section
- **Cabinet Type**: tall (full-height built-in)
- **Components Used**: plywood carcass, adjustable shelving, door hardware, blocking, wall anchors
- **Key Elements**: shelf spacing, door swing, wall blocking, base, crown/header trim
- **Dimensions**: full height to ceiling, 12-24" depth typical
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### BUILT-IN LINEN / PANTRY @ UNITS
- **File**: BUILT-IN LINEN _PANTRY @ UNITS.rvt
- **Type**: section
- **Cabinet Type**: tall (full-height built-in)
- **Components Used**: plywood carcass, adjustable shelving, door hardware, blocking, wall anchors
- **Key Elements**: shelf spacing, door swing, wall blocking, base, crown/header trim
- **Dimensions**: full height to ceiling, 12-24" depth typical
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### BUILT-IN PANTRY / LINEN
- **File**: BUILT-IN PANTRY_ LINEN.rvt
- **Type**: section
- **Cabinet Type**: tall (full-height built-in)
- **Components Used**: plywood carcass, adjustable shelving, blocking, finish trim
- **Key Elements**: shelf layout, door configuration, wall attachment, base detail
- **Dimensions**: full height, standard closet depth
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### CASEWORK / CABINET SECTION - TYPICAL
- **File**: CASEWORK_CABINET SECTION-TYP.rvt
- **Type**: section
- **Cabinet Type**: base (typical casework section)
- **Components Used**: plywood carcass, countertop, adjustable shelves, toe kick, wall blocking
- **Key Elements**: cabinet box construction, countertop attachment, toe kick, wall mounting, shelf standards
- **Dimensions**: 36" AFF countertop, 4" toe kick, 24" depth base, 12" depth upper
- **ADA**: not applicable (standard section)
- **Drawing Complexity**: moderate

### CASEWORK / EXTERIOR GRILLE
- **File**: CASEWORK_EXTERIOR GRILLE1.rvt
- **Type**: section/elevation
- **Cabinet Type**: specialty (exterior grille enclosure)
- **Components Used**: metal grille, frame, blocking, weather-resistant materials
- **Key Elements**: grille pattern, frame attachment, weather seal, ventilation
- **Dimensions**: varies by application
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### CASEWORK / RECEPTION COUNTER
- **File**: CASEWORK_RECEPTION COUNTER.rvt
- **Type**: section
- **Cabinet Type**: specialty (reception/transaction counter)
- **Components Used**: plywood carcass, solid surface top, transaction shelf, knee space framing, wire management
- **Key Elements**: dual-height counter, transaction top, work surface, wire chase, knee space
- **Dimensions**: transaction top 42-44", work surface 29-30", ADA portion 34" max
- **ADA**: ADA-compliant lowered section required with knee clearance
- **Drawing Complexity**: complex

### ENLARGED COUNTERTOP DETAILS @ UNITS
- **File**: ENLARGED COUNTERTOP DETAILS @ UNITS.rvt
- **Type**: section (enlarged)
- **Cabinet Type**: countertop (edge detail)
- **Components Used**: solid surface/stone countertop, plywood substrate, edge profile, backsplash
- **Key Elements**: edge profile, substrate attachment, backsplash connection, overhang dimension
- **Dimensions**: 1-1/2" countertop thickness typical, 1" overhang
- **ADA**: not applicable
- **Drawing Complexity**: simple

### EXTERIOR BAR SINK CABINET / COUNTER
- **File**: EXTERIOR BAR SINK CABINET_COUNTER.rvt
- **Type**: section
- **Cabinet Type**: base (exterior/weather-resistant)
- **Components Used**: marine-grade plywood, stainless sink, exterior-rated countertop, drainage, waterproofing
- **Key Elements**: sink cutout, plumbing rough-in, waterproof membrane, exterior-rated materials
- **Dimensions**: 36" counter height, sink dimensions vary
- **ADA**: not applicable
- **Drawing Complexity**: complex

### LED LIGHT RECESS @ GYM MILLWORK
- **File**: LED LIGHT RECESS @ GYM MILLWORK.rvt
- **Type**: section (detail)
- **Cabinet Type**: specialty (integrated lighting)
- **Components Used**: LED strip channel, millwork reveal, acrylic lens, blocking, wiring chase
- **Key Elements**: LED channel depth, lens detail, reveal dimensions, wiring path
- **Dimensions**: recess depth 1-2", reveal width varies
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### RECESSED SHELVING DETAIL @ UNIT
- **File**: RECESSED SHELVING DETAIL @ UNIT.rvt
- **Type**: section
- **Cabinet Type**: specialty (recessed/niche shelving)
- **Components Used**: framing, plywood liner, shelf supports, drywall return, trim
- **Key Elements**: wall framing opening, shelf support method, drywall edge condition, depth
- **Dimensions**: niche depth 4-6" typical, width varies
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### SHELVING @ CLUBROOM
- **File**: SHELVING @ CLUBROOM.rvt
- **Type**: section/elevation
- **Cabinet Type**: specialty (open shelving system)
- **Components Used**: shelf brackets, wood/metal shelves, wall blocking, anchors
- **Key Elements**: bracket spacing, shelf thickness, wall blocking locations, load capacity
- **Dimensions**: shelf spacing varies, blocking at 16" o.c.
- **ADA**: not applicable
- **Drawing Complexity**: simple

### TYP. CLEARANCE BETWEEN KITCHEN COUNTERS
- **File**: TYP. CLEARANCE BETWEEN KITCHEN COUNTERS.rvt
- **Type**: plan (clearance diagram)
- **Cabinet Type**: base (kitchen layout clearance)
- **Components Used**: base cabinets, countertops, dimension annotations
- **Key Elements**: parallel counter clearance, appliance clearance, door swing zones
- **Dimensions**: 42" min clearance (48" ADA), 36" min one-cook kitchen
- **ADA**: yes - 48" clear between counters for wheelchair access
- **Drawing Complexity**: simple

### TYP. MIN. CLEARANCE IN U-SHAPED KITCHEN
- **File**: TYP. MIN. CLEARANCE IN U-SHAPED KITCHEN.rvt
- **Type**: plan (clearance diagram)
- **Cabinet Type**: base (U-shaped kitchen layout)
- **Components Used**: base cabinets, countertops, dimension annotations
- **Key Elements**: U-shaped counter clearance, appliance zones, work triangle
- **Dimensions**: 60" min inside U-shape, 42-48" between counters
- **ADA**: yes - 60" turning radius within U-shape
- **Drawing Complexity**: simple

---

## Preview-Only Details (no .rvt in removed_2026/)

These details exist as preview images in the library and may have .rvt files in the main library location.

### BASE CABINET (Standard)
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: base
- **Components Used**: plywood carcass, adjustable shelves, toe kick, countertop, blocking
- **Key Elements**: cabinet box, adjustable shelves, toe kick board, countertop edge, wall attachment
- **Dimensions**: 36" AFF countertop, 34-1/2" cabinet, 4-1/2" toe kick, 24" depth
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### UPPER CABINET (Standard)
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: upper
- **Components Used**: plywood carcass, adjustable shelves, door, wall blocking, fasteners
- **Key Elements**: wall mounting, shelf standards, door overlay, crown mold, soffit condition
- **Dimensions**: 18" AFF from countertop, 12" depth, 30-42" height
- **ADA**: max reach 48" AFF for accessible
- **Drawing Complexity**: moderate

### ADA WALL MOUNTED VANITY
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: vanity (wall-mounted ADA)
- **Components Used**: wall blocking, steel bracket/cleat, countertop, undermount sink, insulation wrap on pipes
- **Key Elements**: knee clearance, pipe insulation (burn protection), open front, no cabinet below
- **Dimensions**: 34" max AFF, 27" min knee clearance, 8" min depth at knee, 17" min depth at toe
- **ADA**: yes - full ADA compliance: knee/toe clearance, insulated pipes, reach ranges
- **Drawing Complexity**: moderate

### BA: BASE CABINET WITH SINK
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: base (sink cabinet)
- **Components Used**: plywood carcass, countertop, undermount sink, plumbing, P-trap, supply lines
- **Key Elements**: sink cutout reinforcement, plumbing access, water supply, drain, countertop support
- **Dimensions**: 36" AFF, sink bowl depth varies
- **ADA**: not applicable (standard height)
- **Drawing Complexity**: complex

### BA: ADA BASE CABINET WITH SINK AT PATIENT ROOMS
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: base (ADA sink, healthcare)
- **Components Used**: ADA cabinet, undermount sink, insulated pipes, lever faucet, countertop
- **Key Elements**: knee clearance, pipe insulation, lever-handle faucet, open front, blocking
- **Dimensions**: 34" max AFF, 27" knee clearance, 6" deep toe clearance
- **ADA**: yes - healthcare ADA with insulated supply/drain pipes
- **Drawing Complexity**: complex

### BB: BASE CABINET WITH INTEGRAL SINK
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: base (integral sink)
- **Components Used**: solid surface countertop with integral bowl, plywood substrate, plumbing
- **Key Elements**: integral sink bowl, seamless countertop, drain connection, supply lines
- **Dimensions**: 36" AFF, integral bowl depth per manufacturer
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### BC: DESK WITH COUNTER
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: base (desk/work surface)
- **Components Used**: plywood substrate, laminate top, knee space framing, wire management
- **Key Elements**: work surface, knee space, wire chase, modesty panel, desktop edge
- **Dimensions**: 29-30" AFF work surface, 24" depth
- **ADA**: 27" min knee clearance if ADA workstation
- **Drawing Complexity**: simple

### BD: BASE CABINET WITH DRAWERS
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: base (drawer unit)
- **Components Used**: plywood carcass, drawer slides (full extension), drawer fronts, countertop
- **Key Elements**: drawer slide mounting, drawer box construction, front overlay, pull hardware
- **Dimensions**: 36" AFF, drawer depths vary (4-8" typical)
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### BE: BASE CABINET WITH DOORS
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: base (door cabinet)
- **Components Used**: plywood carcass, hinged doors, adjustable shelf, toe kick, countertop
- **Key Elements**: hinge type, door overlay, shelf supports, interior layout
- **Dimensions**: 36" AFF, 24" depth, single or double door
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### BF: DESK WITH COUNTER (Variant)
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: base (desk variant)
- **Components Used**: plywood substrate, laminate/solid surface top, pedestal support, wire chase
- **Key Elements**: desktop height, pedestal configuration, wire management, edge detail
- **Dimensions**: 29-30" AFF work surface
- **ADA**: 27" min knee clearance
- **Drawing Complexity**: simple

### BF: ADA BASE CABINET WITH SINK
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: base (ADA sink)
- **Components Used**: ADA-compliant cabinet, undermount sink, insulated P-trap, insulated supply
- **Key Elements**: open knee space, pipe insulation, lever faucet, removable base panel
- **Dimensions**: 34" max AFF, 27" knee clearance
- **ADA**: yes - full ADA sink compliance
- **Drawing Complexity**: complex

### BG: BASE CABINET END PANEL
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: base (end condition)
- **Components Used**: exposed end panel, edge banding, filler strip, countertop overhang
- **Key Elements**: end panel material, edge treatment, filler to wall, scribing
- **Dimensions**: flush end or 1/4" overhang, filler 1-3" to wall
- **ADA**: not applicable
- **Drawing Complexity**: simple

### BH: CHECK-IN COUNTER (CHECK-OUT COUNTER SIM.)
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: specialty (transaction counter)
- **Components Used**: dual-height counter, transaction shelf, work surface, structural support column
- **Key Elements**: public side, staff side, transaction shelf height, work surface, wire chase
- **Dimensions**: transaction 42-44", work 29-30", ADA section 34"
- **ADA**: yes - lowered ADA transaction section required
- **Drawing Complexity**: complex

### BK: DESK WITH COUNTER
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: base (desk variant)
- **Components Used**: plywood substrate, laminate top, knee space, grommet, modesty panel
- **Key Elements**: grommet for wiring, modesty panel, desktop height, edge profile
- **Dimensions**: 29-30" AFF
- **ADA**: 27" knee clearance if accessible
- **Drawing Complexity**: simple

### BM: BASE CABINET WITH MICROWAVE SHELF AND DRAWER
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: base (appliance cabinet)
- **Components Used**: plywood carcass, fixed microwave shelf, drawer below, ventilation space, countertop
- **Key Elements**: microwave shelf height, ventilation clearance, drawer below, electrical outlet
- **Dimensions**: microwave shelf at ~15-18" AFF, countertop 36" AFF
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### BP: BASE CABINET PULL-OUT TRASH CONTAINER
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: base (pull-out trash)
- **Components Used**: plywood carcass, full-extension slides, trash bin frame, door-mounted pull-out
- **Key Elements**: slide mounting, bin frame, door attachment, stop mechanism
- **Dimensions**: 36" AFF, 15-18" wide, single or double bin
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### BP: BASE CABINET WITH TRASH CONTAINER
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: base (trash cabinet)
- **Components Used**: plywood carcass, removable bin, tilt-out door, ventilation
- **Key Elements**: bin access, tilt mechanism, ventilation, interior liner
- **Dimensions**: 36" AFF, 15" wide typical
- **ADA**: not applicable
- **Drawing Complexity**: simple

### CABINET ANCHORAGE - FLOOR
- **File**: (preview only)
- **Type**: section (detail)
- **Cabinet Type**: base (anchorage detail)
- **Components Used**: cabinet base, L-bracket, concrete anchor, shim, leveling screws
- **Key Elements**: floor anchor type, shim location, leveling method, seismic anchorage
- **Dimensions**: anchor embedment depth per structural, bracket size
- **ADA**: not applicable
- **Drawing Complexity**: simple

### CABINET ANCHORAGE - WALL
- **File**: (preview only)
- **Type**: section (detail)
- **Cabinet Type**: upper (anchorage detail)
- **Components Used**: hanging rail/cleat, lag screws, wall blocking, cabinet back
- **Key Elements**: blocking location, fastener type, cleat profile, load path
- **Dimensions**: blocking 3/4" plywood min, lag screw embedment per load
- **ADA**: not applicable
- **Drawing Complexity**: simple

### FA: FULL HEIGHT CABINET WITH ADJ. SHELVING
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: tall (full-height)
- **Components Used**: plywood carcass, adjustable shelves, shelf standards, hinged doors, toe kick
- **Key Elements**: shelf standard spacing, fixed vs. adjustable shelves, door configuration
- **Dimensions**: 84-96" height, 24" depth, shelf load varies
- **ADA**: accessible shelving max 48" AFF reach
- **Drawing Complexity**: moderate

### FC: FULL HEIGHT CABINET WITH ADJ. SHELVING (Variant)
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: tall (full-height, open front)
- **Components Used**: plywood carcass, adjustable shelves, shelf standards, no doors
- **Key Elements**: open shelving configuration, load-bearing shelf support, shelf pin spacing
- **Dimensions**: 84-96" height, 12-24" depth
- **ADA**: accessible shelving max 48" AFF reach
- **Drawing Complexity**: moderate

### FULL HEIGHT CABINET SECTION
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: tall (full-height with upper/lower zones)
- **Components Used**: plywood carcass, countertop at mid-height, upper/lower doors, adjustable shelves
- **Key Elements**: mid-height counter, upper cabinet zone, lower cabinet zone, blocking
- **Dimensions**: full height to soffit, counter at 36" AFF
- **ADA**: not applicable
- **Drawing Complexity**: complex

### FURR DOWN ABOVE WALL CABINET OR TALL CABINET
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: upper/tall (soffit/furr-down)
- **Components Used**: metal stud framing, GWB, cabinet top, blocking, crown mold
- **Key Elements**: furr-down framing to structure above, GWB finish, trim transition to cabinet
- **Dimensions**: furr-down depth varies, closes gap between cabinet top and ceiling
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### INTERIOR - FIRE EXTINGUISHER CABINET
- **File**: (preview only)
- **Type**: section (two conditions: non-rated and 1-hour rated wall)
- **Cabinet Type**: specialty (fire extinguisher)
- **Components Used**: metal cabinet, glass/break-glass door, recessed frame, blocking
- **Key Elements**: wall recess depth, cabinet trim frame, mounting height, clearance to FE
- **Dimensions**: 6-8" recess depth, mounting per NFPA 10 (max 5' AFF to top, 4" min AFF)
- **ADA**: max 48" AFF reach, operable hardware
- **Drawing Complexity**: simple

### INTERIOR - RECESSED FIRE EXTINGUISHER CABINET
- **File**: (preview only)
- **Type**: section (head and sill conditions)
- **Cabinet Type**: specialty (recessed fire extinguisher)
- **Components Used**: metal cabinet, recessed frame, blocking header, trim
- **Key Elements**: header framing, sill condition, recess depth, trim profile
- **Dimensions**: full recess in wall, header and sill framing details
- **ADA**: max 48" AFF to handle
- **Drawing Complexity**: moderate

### RECESSED METAL WALL CABINETS (>16 sq. in. face)
- **File**: (preview only)
- **Type**: section (fire-rated enclosure)
- **Cabinet Type**: specialty (fire-rated recessed cabinet)
- **Components Used**: 5-sided rated enclosure, metal cabinet, Type X GWB, rated framing
- **Key Elements**: 1-hour rated 5-sided enclosure, metallic box max 20" deep x 56" high
- **Dimensions**: 20" max depth, 5-1/4" max depth alternate, 56" max height
- **ADA**: not applicable
- **Drawing Complexity**: complex

### SINK AT COUNTER TOP
- **File**: (preview only)
- **Type**: section (enlarged detail)
- **Cabinet Type**: countertop (sink mounting)
- **Components Used**: countertop, undermount clips, plumber's putty/silicone, plywood substrate, sink
- **Key Elements**: undermount attachment, substrate reinforcement, waterproofing at cutout, plumbing connections
- **Dimensions**: 1-1/2" countertop typical, cutout per sink template
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### TYPICAL COUNTERTOP EDGE DETAIL
- **File**: (preview only)
- **Type**: section (enlarged detail)
- **Cabinet Type**: countertop (edge profile)
- **Components Used**: solid surface/stone countertop, buildup strip, substrate
- **Key Elements**: edge profile (1/2" solid surface), 3/4" plywood substrate, buildup for thick edge
- **Dimensions**: 1/2" solid surface + 3/4" substrate, 1/4" overhang past cabinet face
- **ADA**: not applicable
- **Drawing Complexity**: simple

### TYPICAL UPPER CABINET DETAIL
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: upper (typical mounting detail)
- **Components Used**: plywood carcass, hanging rail, lag screws, wall blocking, GWB, structural wall
- **Key Elements**: hanging rail/cleat at top, screws through back into blocking, shelf standards, door
- **Dimensions**: 12" depth, 30-42" height, 18" above countertop, blocking required
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### WA: UPPER CABINET
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: upper (standard with doors)
- **Components Used**: plywood carcass, hinged doors, adjustable shelves, wall mounting cleat
- **Key Elements**: door overlay, shelf pin holes, back panel, top nailer, wall attachment
- **Dimensions**: 12" depth, 30" or 42" height
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### WB: UPPER CABINET WITHOUT DOORS
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: upper (open shelving)
- **Components Used**: plywood carcass, adjustable shelves, wall mounting cleat, exposed edges
- **Key Elements**: edge banding on exposed edges, open front, shelf supports
- **Dimensions**: 12" depth, 30" height typical
- **ADA**: not applicable
- **Drawing Complexity**: simple

### WB: UPPER CABINET WITH MICROWAVE
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: upper (microwave housing)
- **Components Used**: plywood carcass, microwave bracket, ventilation space, electrical rough-in
- **Key Elements**: microwave mounting bracket, vent above, shelf above, electrical outlet location
- **Dimensions**: microwave opening per manufacturer, 18" above countertop
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### WC: UPPER CABINET OPEN FROM BELOW
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: upper (open-bottom specialty)
- **Components Used**: plywood carcass, fixed bottom shelf, blocking, concealed fasteners
- **Key Elements**: open bottom for display/access, blocking for overhead attachment, lighting slot
- **Dimensions**: 12" depth, open bottom zone 6-12" height
- **ADA**: not applicable
- **Drawing Complexity**: moderate

### WE: UPPER CABINET WITH MICROWAVE (Variant)
- **File**: (preview only)
- **Type**: section
- **Cabinet Type**: upper (over-range microwave)
- **Components Used**: plywood carcass, microwave mounting plate, vent hood connection, electrical
- **Key Elements**: over-range mounting, vent duct connection, structural support for weight, cabinet above
- **Dimensions**: 30" above cooktop min, microwave per manufacturer
- **ADA**: not applicable
- **Drawing Complexity**: complex

### 5-SIDED ENCLOSURE (1-HR Rated Barrier for Electrical Cabinets)
- **File**: (preview only)
- **Type**: section/notes (code detail)
- **Cabinet Type**: specialty (fire-rated enclosure)
- **Components Used**: Type X GWB, rated framing, fire caulk, metallic cabinet box
- **Key Elements**: 1-hour fire-rated construction, 5-sided GWB enclosure around metallic cabinets
- **Dimensions**: max 20" depth x 5-1/4" max depth x 56" max height
- **ADA**: not applicable
- **Drawing Complexity**: moderate

---

## Summary Statistics

| Cabinet Type | Count |
|-------------|-------|
| Base | 15 |
| Upper | 10 |
| Tall/Full-Height | 5 |
| Specialty | 9 |
| Countertop | 3 |
| Vanity | 1 |
| **Total** | **43** |

| ADA Details | Count |
|------------|-------|
| ADA-compliant | 8 |
| Standard (non-ADA) | 35 |

| Drawing Type | Count |
|-------------|-------|
| Section | 36 |
| Plan/Clearance | 2 |
| Detail (enlarged) | 3 |
| Notes/Code | 2 |
