# Cursor

Cursor can connect in two ways:

- Stdio: `uvx kicad-mcp-pro`
- HTTP: local bridge + `http://127.0.0.1:<port>/mcp`

For larger tool surfaces, it is often helpful to set `KICAD_MCP_PROFILE=pcb_only`, `schematic_only`, or `high_speed`.
