AgentDeck · Gallery

# The hardware

Every surface AgentDeck steers, board by board. Photos are added one at a time — empty slots show the hatch placeholder with the filename to drop in.

Specs mirror the hardware spec sheet (SSOT: `docs/hardware-compatibility.md`). Add a photo at `docs/gallery/photos/<slug>.jpg`.

## ESP32 firmware displays

Photo slot photos/ips35.jpg

### IPS 3.5"

ESP32-S3

JC3248W535 · Guition

Resolution 480×320
Panel AXS15231B IPS
Transport Serial / WiFi WS
Photo slot photos/amoled18.jpg

### Round AMOLED 1.8"

ESP32-S3

JC3636W518 · Guition

Resolution 360×360
Panel ST77916 AMOLED
Transport Serial / WiFi WS
Photo slot photos/box86.jpg

### 86 Box 4"

ESP32-S3

ESP32-S3-4848S040 · Guition

Resolution 480×480
Panel ST7701 IPS
Transport Serial / WiFi WS
Photo slot photos/ttgo.jpg

### TTGO T-Display 1.14"

ESP32

LilyGO T-Display

Resolution 135×240
Panel ST7789 TFT
Transport Serial / WiFi WS
Photo slot photos/ips10.jpg

### IPS 10.1"

ESP32-P4 + C6

JC8012P4A1C · Guition

Resolution 800×1280
Panel JD9365 MIPI-DSI
Transport Serial / WiFi WS
Photo slot photos/inkdeck.jpg

### InkDeck e-ink

EXPERIMENTAL

Seeed TRMNL 7.5" OG · XIAO ESP32-S3 Plus

Resolution 800×480
Panel UC8179 e-ink
Transport WiFi WS (planned)
Photo slot photos/xteink-x3.jpg

### XTeink X3

EXPERIMENTAL

ESP32-C3 · CrossPoint Reader fork

Resolution 528×792
Panel 3.7" e-ink
Transport WiFi WS

## LED matrices

Photo slot photos/pixoo64.jpg

### Divoom Pixoo64

LED

Commercial LED frame · WiFi

Resolution 64×64 RGB
Transport HTTP REST :80
Connect WiFi 2.4G
Photo slot photos/tc001.jpg

### Ulanzi TC001

ESP32

WS2812B matrix · env led8x32

Resolution 8×32 (256 LED)
Render FastLED 3.7
Transport Serial / WiFi WS
Photo slot photos/idotmatrix.jpg

### iDotMatrix 32×32

BLE

Commercial BLE pixel display

Resolution 32×32 AMOLED
Transport BLE GATT
Connect Bluetooth LE
Photo slot photos/timebox-mini.jpg

### Divoom Timebox Mini

BLE

Commercial BLE pixel display

Resolution 11×11 RGB
Transport BLE GATT (ISSC)
Connect Bluetooth LE

## HID decks

Photo slot photos/d200h.jpg

### Ulanzi D200H

HID

SigmaStar SSD210 · Deck Dock

Resolution 960×540
Keys 14 (nv3052c LCD)
Transport Ulanzi Studio plugin
Photo slot photos/streamdeck-plus.jpg

### Stream Deck+

HID

Elgato · agentdeck-sdplus

Keys 8 (4×2)
Input 4 dials + touch strip
Transport WebSocket :9120
Photo slot photos/streamdeck-15.jpg

### Stream Deck (15-key)

HID

Elgato · agentdeck-sd

Keys 15 (5×3)
Also mini · XL auto-grid
Transport WebSocket :9120

## Software & terminal surfaces

Screenshot slot photos/macos.jpg

### Apple — macOS

SwiftUI

In-process Swift daemon · App Store

Min OS macOS 26.0
Daemon in-process :9120
Bundle agent.deck
Screenshot slot photos/ios.jpg

### Apple — iOS / iPadOS

SwiftUI

Same-LAN WebSocket viewer

Min OS iOS / iPadOS 17
Transport WebSocket :9120
Connect WiFi (same-LAN)
Screenshot slot photos/android-eink.jpg

### Android — e-ink

Compose

Crema / Onyx / Kobo / Pantone

Refresh GC16 / DU / A2
Transport WS (ADB localhost)
minSdk 29
Screenshot slot photos/android-tablet.jpg

### Android — tablet

Compose

Color LCD launcher

Render 60fps color
Transport WS + mDNS
Connect WiFi (same-LAN)
Screenshot slot photos/tui.jpg

### TUI Dashboard

terminal

`agentdeck dashboard`

Render truecolor ANSI
Terrarium braille sprites
Transport WebSocket :9120