RAIL PLASMA thruster design engine
T: 0 mN ISP: 0 s ve: 0 km/s P: 0 W η: 0% ṁ: 0 mg/s
click tube to place coil · drag to move · scroll = strength · DEL remove
Geometry
Cathode r5 mm
Anode r25 mm
Length80 mm
Nozzle50%
Operating Point
Current200 A
Mass flow10 mg/s
B applied0.10 T
Gas
40.0 AMU
View
Field
Overlay
Presets
Validation vs Published Data
Parameter Sweep
Sweep
Min10
Max90
Hardware Specification
Thrust Breakdown
—
Simulate
Validate
Optimize
Spec
RAIL PLASMA v2 — SI calibrated