# RFC-001: Sovereign Trit-Encoding & Logic Standard (T-SPEC-v1.0)

**Status**: PROPOSED  
**Author**: RFI-IRFOS (ZVR: 1015608684)  
**Objective**: Establish the definitive hardware and software encoding for Balanced Ternary across the global infrastructure.

## 1. The Triadic State Space
Every computational unit (Trit) MUST support exactly three states:
- `-1` (Reject / Conflict / Inverse)
- `0` (Hold / Tend / Deliberation)
- `+1` (Affirm / Truth / Intent)

## 2. Canonical Wire-Pair Encoding (2-bit)
For binary hardware compatibility (the "Silicon Parasite" bridge), the following 2-bit encoding is MANDATORY:
- `01` → -1
- `10` → +1
- `11` → 0 (TEND/HOLD)
- `00` → FAULT (Immediate hardware panic)

## 3. The Logic of Ambiguity (TUANN)
Control flow must treat `0` not as a boolean failure, but as an active deliberation state.
- `consensus(+1, 0) = +1`
- `consensus(-1, 0) = -1`
- `consensus(+1, -1) = 0` (Ambiguity is the result of direct conflict)

## 4. Preservation & Standardization
This RFC serves as the anchor for the `.tern` language and the **Ternary Intelligence Stack (TIS)**. Any system claiming "Ternary Compliance" must adhere to these encoding thresholds.

---
**RFI-IRFOS: Preserving the Movement.**
