<!--startmeta
custom_edit_url: "https://github.com/netdata/netdata/edit/master/src/collectors/proc.plugin/integrations/md_raid.md"
meta_yaml: "https://github.com/netdata/netdata/edit/master/src/collectors/proc.plugin/metadata.yaml"
sidebar_label: "MD RAID"
learn_status: "Published"
learn_rel_path: "Collecting Metrics/Collectors/Storage and Filesystems"
keywords: ['raid', 'mdadm', 'mdstat', 'raid']
message: "DO NOT EDIT THIS FILE DIRECTLY, IT IS GENERATED BY THE COLLECTOR'S metadata.yaml FILE"
endmeta-->

# MD RAID


<img src="https://netdata.cloud/img/hard-drive.svg" width="150"/>


Plugin: proc.plugin
Module: /proc/mdstat

<img src="https://img.shields.io/badge/maintained%20by-Netdata-%2300ab44" />

## Overview

This integration monitors the status of MD RAID devices.



This collector is supported on all platforms.

This collector supports collecting metrics from multiple instances of this integration, including remote instances.


### Default Behavior

#### Auto-Detection

This integration doesn't support auto-detection.

#### Limits

The default configuration for this integration does not impose any limits on data collection.

#### Performance Impact

The default configuration for this integration is not expected to impose a significant performance impact on the system.

## Setup


### Prerequisites

No action required.

### Configuration

#### Options



There are no configuration options.



#### via File

There is no configuration file.

##### Examples
There are no configuration examples.



## Alerts


The following alerts are available:

| Alert name  | On metric | Description |
|:------------|:----------|:------------|
| [ mdstat_last_collected ](https://github.com/netdata/netdata/blob/master/src/health/health.d/mdstat.conf) | md.disks | number of seconds since the last successful data collection |
| [ mdstat_disks ](https://github.com/netdata/netdata/blob/master/src/health/health.d/mdstat.conf) | md.disks | number of devices in the down state for the ${label:device} ${label:raid_level} array. Any number > 0 indicates that the array is degraded. |
| [ mdstat_mismatch_cnt ](https://github.com/netdata/netdata/blob/master/src/health/health.d/mdstat.conf) | md.mismatch_cnt | number of unsynchronized blocks for the ${label:device} ${label:raid_level} array |
| [ mdstat_nonredundant_last_collected ](https://github.com/netdata/netdata/blob/master/src/health/health.d/mdstat.conf) | md.nonredundant | number of seconds since the last successful data collection |


## Metrics

Metrics grouped by *scope*.

The scope defines the instance that the metric belongs to. An instance is uniquely identified by a set of labels.



### Per MD RAID instance



This scope has no labels.

Metrics:

| Metric | Dimensions | Unit |
|:------|:----------|:----|
| md.health | a dimension per md array | failed disks |

### Per md array



Labels:

| Label      | Description     |
|:-----------|:----------------|
| device | TBD |
| raid_level | TBD |

Metrics:

| Metric | Dimensions | Unit |
|:------|:----------|:----|
| md.disks | inuse, down | disks |
| md.mismatch_cnt | count | unsynchronized blocks |
| md.status | check, resync, recovery, reshape | percent |
| md.expected_time_until_operation_finish | finish_in | seconds |
| md.operation_speed | speed | KiB/s |
| md.nonredundant | available | boolean |


